(footprint "QFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "QFN, 24 Pin (http://www.alfarzpp.lv/eng/sc/AS3330.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "QFN NoLead")
	(property "Reference" "U14"
		(at 0 -3.33 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "b313b324-ef01-46fd-9e19-fad52a3ae8eb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "FE1.1S-BQFN24B"
		(at 0 3.33 0)
		(layer "F.Fab")
		(uuid "f5753b36-fcee-47b3-afb8-90f5beb89353")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2fc084da-fb6a-45f4-8b76-346b20f8f6db")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2306141021_Terminus-Tech-FE1-1S-BQFN24B_C6776948.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "09116c9c-1722-4e66-b941-b58123fd44df")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b77b6c34-40f0-48d7-b5dc-e08a15442490")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C6776948"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "4728ac5d-fa6a-464f-9910-81af8b549919")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "Terminus Tech"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "373204ce-019e-4a9a-8451-5bfbea6e56b4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "FE1.1S-BQFN24B"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "da3cae61-f882-4ca4-98bc-082d0ee1f163")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.11 -1.635)
		(end -2.11 -1.87)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "cc86d1af-55aa-41d2-a5e9-6e0132d0278c")
	)
	(fp_line
		(start -2.11 2.11)
		(end -2.11 1.635)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "430566e8-2c7e-4a3a-9859-82ec4502bc6e")
	)
	(fp_line
		(start -1.635 -2.11)
		(end -1.81 -2.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "106ae742-94ca-404c-ad82-e79c1b6b9299")
	)
	(fp_line
		(start -1.635 2.11)
		(end -2.11 2.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3565cfa3-c25a-4f62-b611-68d4fc0770ea")
	)
	(fp_line
		(start 1.635 -2.11)
		(end 2.11 -2.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4533cbfa-71d2-4ec9-bc8a-1254119db7d7")
	)
	(fp_line
		(start 1.635 2.11)
		(end 2.11 2.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ef83b58e-cf4d-45dd-a767-660a246cb3d6")
	)
	(fp_line
		(start 2.11 -2.11)
		(end 2.11 -1.635)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a1ddbf9c-5730-4689-938b-25bc81d58d41")
	)
	(fp_line
		(start 2.11 2.11)
		(end 2.11 1.635)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c836f64b-154e-4767-acf9-5b610f0a7f5f")
	)
	(fp_poly
		(pts
			(xy -2.11 -2.11) (xy -2.35 -2.44) (xy -1.87 -2.44) (xy -2.11 -2.11)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "1c574a41-f7c4-46d4-b1a1-f16de61c028f")
	)
	(fp_line
		(start -2.4 -1.3)
		(end -2.4 1.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "02e5e62b-e8d8-4432-8aad-3d05d489bc4a")
	)
	(fp_line
		(start -2.25 -2)
		(end -2.242848 -1.532119)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "a534d66b-9583-4195-b32f-3ec420bbed34")
	)
	(fp_line
		(start -2.25 2)
		(end -2.242848 1.532119)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "75bbc232-d433-4a17-bfc4-07892c88b9be")
	)
	(fp_line
		(start -2 -2.25)
		(end -1.532119 -2.242848)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "544e0480-a53f-4be1-a524-dd703a538656")
	)
	(fp_line
		(start -2 2.25)
		(end -1.532119 2.242848)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "8a6e1f00-ae39-4ff1-ada6-ab77f984e369")
	)
	(fp_line
		(start -1.3 -2.4)
		(end 1.3 -2.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "4eb5c864-ccdc-4713-b59a-927e51a6b0ee")
	)
	(fp_line
		(start -1.3 2.4)
		(end 1.3 2.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "553cdafb-0529-4be8-b474-f4f42b02107a")
	)
	(fp_line
		(start 2 -2.25)
		(end 1.532119 -2.242848)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "418f3c3a-aa80-4133-bb27-d4b4c10b6774")
	)
	(fp_line
		(start 2 2.25)
		(end 1.532119 2.242848)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "db220800-47ca-41d5-b9ea-c0cd186b3480")
	)
	(fp_line
		(start 2.25 -2)
		(end 2.242848 -1.532119)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ca4aaf3f-9a8e-4aa1-8764-00af18565e64")
	)
	(fp_line
		(start 2.25 2)
		(end 2.242848 1.532119)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "6257f954-1c57-4929-9c89-83cef6f0fc77")
	)
	(fp_line
		(start 2.4 -1.3)
		(end 2.4 1.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "91ae064f-b2f8-4f12-bb13-8aa37fe4f187")
	)
	(fp_arc
		(start -2.4 -1.3)
		(mid -2.357017 -1.440157)
		(end -2.242848 -1.532119)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "137a8f38-0326-4e07-969e-e5563d0dccda")
	)
	(fp_arc
		(start -2.25 -2)
		(mid -2.176777 -2.176777)
		(end -2 -2.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "b2bba8c2-e831-4e66-8317-eeb0be6a8b6d")
	)
	(fp_arc
		(start -2.242848 1.532119)
		(mid -2.357017 1.440157)
		(end -2.4 1.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "7f5ec906-f578-4b3e-bd99-4148c0b3a2e8")
	)
	(fp_arc
		(start -2 2.25)
		(mid -2.176777 2.176777)
		(end -2.25 2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5b13fa8b-392e-4028-93b0-f92cea4453fa")
	)
	(fp_arc
		(start -1.532119 -2.242848)
		(mid -1.440157 -2.357017)
		(end -1.3 -2.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ed7586a8-cb4b-482f-8e36-143097b3c8d3")
	)
	(fp_arc
		(start -1.3 2.4)
		(mid -1.440157 2.357017)
		(end -1.532119 2.242848)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9fe78ed2-1c63-4815-82f1-4869331f0f33")
	)
	(fp_arc
		(start 1.3 -2.4)
		(mid 1.440157 -2.357017)
		(end 1.532119 -2.242848)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "08cbe3ce-4242-4089-af71-47828e80524f")
	)
	(fp_arc
		(start 1.532119 2.242848)
		(mid 1.440157 2.357017)
		(end 1.3 2.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e915ac0e-227f-40f9-adc4-75dc2acbbe4a")
	)
	(fp_arc
		(start 2 -2.25)
		(mid 2.176777 -2.176777)
		(end 2.25 -2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "57ecaf15-3d5c-4174-8fa7-db0dee155a9c")
	)
	(fp_arc
		(start 2.242848 -1.532119)
		(mid 2.357017 -1.440157)
		(end 2.4 -1.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "2d6a498e-10f9-4c44-bb03-78a90b791d02")
	)
	(fp_arc
		(start 2.25 2)
		(mid 2.176777 2.176777)
		(end 2 2.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "66b2d9d5-1fee-4eca-801c-fb601242f385")
	)
	(fp_arc
		(start 2.4 1.3)
		(mid 2.357017 1.440157)
		(end 2.242848 1.532119)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "8ba7a2b0-ca0f-491f-8b6f-06bc12cc9b11")
	)
	(fp_line
		(start -2 -2)
		(end 2 -2)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "becde7ba-7069-40a6-a4ad-e8bc1780ce48")
	)
	(fp_line
		(start -2 -1)
		(end -1 -2)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "08233255-86ee-438a-9022-e5c0e228c112")
	)
	(fp_line
		(start -2 2)
		(end -2 -2)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "fc243e98-f987-4d1c-ab21-8ded74d5b2b6")
	)
	(fp_line
		(start 2 -2)
		(end 2 2)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "938166b5-dfba-44cd-97cd-c13c987eab24")
	)
	(fp_line
		(start 2 2)
		(end -2 2)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "55a0d7e8-3364-40c5-9f79-6fb2221632f0")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "5a56cac3-aaba-42d0-80d9-6da7794dfae0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" smd oval
		(at -1.9 -1.25)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "c7e6c6e9-0004-4390-894e-e67bad12bfe6")
	)
	(pad "" smd oval
		(at -1.9 -0.75)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "72527227-9fd6-498e-b238-113da2d57d56")
	)
	(pad "" smd oval
		(at -1.9 -0.25)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "a23b1ba8-efe5-45ae-a7d5-68e30f9f0bce")
	)
	(pad "" smd oval
		(at -1.9 0.25)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "55c77787-cae3-482b-a300-bbf0cd1e9649")
	)
	(pad "" smd oval
		(at -1.9 0.75)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "89f3780b-3379-4e4e-9fc0-ec9715396285")
	)
	(pad "" smd oval
		(at -1.9 1.25)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "4020e1b5-fde0-4558-895f-f33edab43f30")
	)
	(pad "" smd oval
		(at -1.25 -1.9 270)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "5ff5921d-e8be-4479-a0ab-904132187876")
	)
	(pad "" smd oval
		(at -1.25 1.9 90)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "a42c9817-7906-4cbd-bb3c-efd606276dc2")
	)
	(pad "" smd oval
		(at -0.75 -1.9 270)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "7f9b3761-f5d2-469d-ba8c-f9a86e6c7d2b")
	)
	(pad "" smd oval
		(at -0.75 1.9 90)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "efbd1e7d-68b8-4b9c-ae6c-8b7d3f041b58")
	)
	(pad "" smd roundrect
		(at -0.675 -0.675)
		(size 1.09 1.09)
		(layers "F.Paste")
		(roundrect_rratio 0.229358)
		(uuid "7b4ad959-fc77-490a-b42e-44feda39f5d4")
	)
	(pad "" smd roundrect
		(at -0.675 0.675)
		(size 1.09 1.09)
		(layers "F.Paste")
		(roundrect_rratio 0.229358)
		(uuid "225e6367-939f-497f-bb5e-a3798d747bbc")
	)
	(pad "" smd oval
		(at -0.25 -1.9 270)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "d8036375-b6c4-424b-997a-b2ba7f03b740")
	)
	(pad "" smd oval
		(at -0.25 1.9 90)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "6ba9a178-04d9-4328-aec5-4ed584fae84b")
	)
	(pad "" smd oval
		(at 0.25 -1.9 270)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "acb91c79-d539-46ee-b35a-160ab17d62c7")
	)
	(pad "" smd oval
		(at 0.25 1.9 90)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "5590b876-ba93-4019-b083-c7b007ba2efa")
	)
	(pad "" smd roundrect
		(at 0.675 -0.675)
		(size 1.09 1.09)
		(layers "F.Paste")
		(roundrect_rratio 0.229358)
		(uuid "6a140da9-cc2c-4ac7-89e3-69ba9595b04a")
	)
	(pad "" smd roundrect
		(at 0.675 0.675)
		(size 1.09 1.09)
		(layers "F.Paste")
		(roundrect_rratio 0.229358)
		(uuid "cbc2fd4c-7971-4b75-a92b-ac17e5d1bea4")
	)
	(pad "" smd oval
		(at 0.75 -1.9 270)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "ca09e7dd-28cd-4844-ae7b-9d3fc2f94d27")
	)
	(pad "" smd oval
		(at 0.75 1.9 90)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "3f304f17-7db1-45c0-83c4-34598a84a73f")
	)
	(pad "" smd oval
		(at 1.25 -1.9 270)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "cd0f076a-0484-4919-a5d2-b43f6151fdfe")
	)
	(pad "" smd oval
		(at 1.25 1.9 90)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "30d7532a-5d19-4c47-8c17-8427a337f321")
	)
	(pad "" smd oval
		(at 1.9 -1.25 180)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "3bebcdf6-36c8-4341-9c24-7fccdc706f9b")
	)
	(pad "" smd oval
		(at 1.9 -0.75 180)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "c420075a-a18b-4cbb-82dd-8e3c6d7871da")
	)
	(pad "" smd oval
		(at 1.9 -0.25 180)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "c78fa904-033f-47c8-b313-779b6c0afa77")
	)
	(pad "" smd oval
		(at 1.9 0.25 180)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "0a406a2d-6983-4d52-a610-24aa6d069efc")
	)
	(pad "" smd oval
		(at 1.9 0.75 180)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "59b6eb82-aa40-442c-b89e-9aa983a1bba2")
	)
	(pad "" smd oval
		(at 1.9 1.25 180)
		(size 0.6 0.2)
		(layers "F.Paste")
		(uuid "36b4e1cf-5779-4ffb-ba00-839c57bb4c84")
	)
	(pad "1" smd roundrect
		(at -1.9 -1.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "235ac93d-79cd-44d1-a55a-2281d9882ac3")
	)
	(pad "2" smd roundrect
		(at -1.9 -0.75)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "a03f94b4-a74b-4f95-a376-b1b2f17da10f")
	)
	(pad "3" smd roundrect
		(at -1.9 -0.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "e1e85a38-4bb0-4875-b064-a68beae36d7a")
	)
	(pad "4" smd roundrect
		(at -1.9 0.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "c5f0630c-560f-4dee-92f8-c2115d75c38b")
	)
	(pad "5" smd roundrect
		(at -1.9 0.75)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "ea499c6a-4516-4961-aa0b-481a4871ef5c")
	)
	(pad "6" smd roundrect
		(at -1.9 1.25)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "c7990413-2a39-4e3e-9253-2e20bf673eeb")
	)
	(pad "7" smd roundrect
		(at -1.25 1.9 90)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "078c96fe-9fce-4c9e-93af-084df77b6e13")
	)
	(pad "8" smd roundrect
		(at -0.75 1.9 90)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "22f674aa-dde2-47ab-aff7-2ec27cb3f88a")
	)
	(pad "9" smd roundrect
		(at -0.25 1.9 90)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "21e3d5ca-d17b-4de5-8564-a0f07b08b633")
	)
	(pad "10" smd roundrect
		(at 0.25 1.9 90)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "9f4b830d-6020-41da-abbc-6cff7a256b6d")
	)
	(pad "11" smd roundrect
		(at 0.75 1.9 90)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "8f0644f0-0d68-406c-9d16-0a16f6b04bdd")
	)
	(pad "12" smd roundrect
		(at 1.25 1.9 90)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "59d18d81-bccb-40e3-b219-5f77d8e58a0d")
	)
	(pad "13" smd roundrect
		(at 1.9 1.25 180)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "440f7a7a-1379-483b-bc51-52374d0fbb91")
	)
	(pad "14" smd roundrect
		(at 1.9 0.75 180)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "06ef42d0-a034-415d-90e1-774d3fcfd148")
	)
	(pad "15" smd roundrect
		(at 1.9 0.25 180)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "80f8e6ee-5904-4f65-9cfa-a51bfa2cacd8")
	)
	(pad "16" smd roundrect
		(at 1.9 -0.25 180)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "8266b1f5-2c92-4ff1-bdaa-eda3395e472f")
	)
	(pad "17" smd roundrect
		(at 1.9 -0.75 180)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "a370ec71-a7b3-4c5d-92cc-5c566a9e7065")
	)
	(pad "18" smd roundrect
		(at 1.9 -1.25 180)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "23ef0544-19d1-4c0b-a500-936b3431047a")
	)
	(pad "19" smd roundrect
		(at 1.25 -1.9 270)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "6dc65727-96c4-4f77-b06e-e63a1f938add")
	)
	(pad "20" smd roundrect
		(at 0.75 -1.9 270)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "26f5fd30-4178-42de-a99c-df6e6b7a3c69")
	)
	(pad "21" smd roundrect
		(at 0.25 -1.9 270)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "eb24ecb6-de06-4454-bf47-dded273f2cfc")
	)
	(pad "22" smd roundrect
		(at -0.25 -1.9 270)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "e1e370fd-d58c-410f-abf1-5c02011ef5de")
	)
	(pad "23" smd roundrect
		(at -0.75 -1.9 270)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "49b75b49-82a1-4b72-859d-08a445839dff")
	)
	(pad "24" smd roundrect
		(at -1.25 -1.9 270)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(uuid "eecbd065-e6bb-49dd-aad6-cdeaea5988d2")
	)
	(pad "25" smd roundrect
		(at 0 0)
		(size 2.7 2.7)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.01851851852)
		(zone_connect 2)
		(uuid "59ba94cc-237c-4c15-a2d7-f441b289ba3d")
	)
	(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
