(footprint "L_Sunlord_SWPA5040S"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Inductor, Sunlord, SWPA5040S, 5.0x5.0x4.0mm, https://www.sunlordinc.com/UploadFiles/PDF_Cat/20120704094224784.pdf")
	(tags "Inductor swpa")
	(property "Reference" "L2"
		(at 0 -3.5 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "3516c6b3-b7b8-47ac-a870-62e5a07d9ff4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "3.3uH"
		(at 0 3.5 0)
		(layer "F.Fab")
		(uuid "1c1fbfbd-c9b6-4c0f-91b9-b507d689c862")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Inductor_SMD:L_Sunlord_SWPA5040S"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "f726598a-5434-457e-b037-768be8fafc09")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "21ea815f-2402-41fb-96ab-16fe2fa98e2e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "67bbcc3b-f9f2-486f-8b75-59ecfc30c1ce")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "d14a7715-2ae5-47c9-bac9-038f8ea30cc4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "7e13303f-2800-49cf-91f7-b39b0cf9c88c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "90bc6b17-347d-4e4b-a100-aee72c2a5820")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.76 -2.76)
		(end -2.76 -2.36)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "cda50ca6-ddc6-4e77-b809-be38ac3ddf92")
	)
	(fp_line
		(start -2.76 -2.76)
		(end 2.76 -2.76)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "77e918ea-89af-4d2f-b49c-b7b280afebf6")
	)
	(fp_line
		(start -2.76 2.76)
		(end -2.76 2.36)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2954d180-66b9-43a8-bf3a-c8b5de85249b")
	)
	(fp_line
		(start -2.76 2.76)
		(end 2.76 2.76)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6a7536c4-563b-4a6e-9b6a-49c24e6d552f")
	)
	(fp_line
		(start 2.76 -2.76)
		(end 2.76 -2.36)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9d266f7c-8600-4c03-b0e6-814fbbdf1507")
	)
	(fp_line
		(start 2.76 2.76)
		(end 2.76 2.36)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "834bd691-0090-44d5-abfb-a77499ed01d2")
	)
	(fp_line
		(start -2.75 2.5)
		(end -2.75 -2.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "4a47e50d-5f4b-40af-bb36-0cd4ff052d76")
	)
	(fp_line
		(start -2.5 -2.75)
		(end 2.5 -2.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f54d9826-2e8f-40f1-b0b4-c3ca1f320464")
	)
	(fp_line
		(start 2.5 2.75)
		(end -2.5 2.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "8b69b6da-18e2-4d7e-9089-61cd9dec166d")
	)
	(fp_line
		(start 2.75 -2.5)
		(end 2.75 2.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "87a46dcb-a27d-4caf-ab74-0acc56087d0d")
	)
	(fp_arc
		(start -2.75 -2.5)
		(mid -2.676777 -2.676777)
		(end -2.5 -2.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "18f76924-6f8b-4838-908b-e7fdc07f37ad")
	)
	(fp_arc
		(start -2.5 2.75)
		(mid -2.676777 2.676777)
		(end -2.75 2.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "325148ad-01c0-4ee2-b681-1f11ba627070")
	)
	(fp_arc
		(start 2.5 -2.75)
		(mid 2.676777 -2.676777)
		(end 2.75 -2.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "738bfce4-fc10-47bb-97b1-941aee10a43a")
	)
	(fp_arc
		(start 2.75 2.5)
		(mid 2.676777 2.676777)
		(end 2.5 2.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "7ea4e3bf-f45e-459e-a3af-8b15f435304d")
	)
	(fp_line
		(start -2.5 -2.5)
		(end -2.5 2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3fad7542-c1d6-4103-84a5-b0fa1ab75ec2")
	)
	(fp_line
		(start -2.5 2.5)
		(end 2.5 2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "79624e45-87e2-42ee-a722-1516e0b1db44")
	)
	(fp_line
		(start 2.5 -2.5)
		(end -2.5 -2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "188d074b-d1a6-4ec5-8b0c-82b425f71ffc")
	)
	(fp_line
		(start 2.5 2.5)
		(end 2.5 -2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8da9ae2c-40ad-4c3c-9de4-75f843d0b05d")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "7b547e8f-2b71-484d-9f4c-7bf9074c8a0d")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.075)
			)
		)
	)
	(pad "" smd roundrect
		(at -1.85 -1.1)
		(size 1.4 2)
		(layers "F.Paste")
		(roundrect_rratio 0.1785714286)
		(uuid "8d46697a-7e70-449d-9ec7-139ee78c11ae")
	)
	(pad "" smd roundrect
		(at -1.85 1.1)
		(size 1.4 2)
		(layers "F.Paste")
		(roundrect_rratio 0.1785714286)
		(uuid "0fb4da84-d1f1-4794-bbef-6f68f4f0ca8a")
	)
	(pad "" smd roundrect
		(at 1.85 -1.1)
		(size 1.4 2)
		(layers "F.Paste")
		(roundrect_rratio 0.1785714286)
		(uuid "7048c4ad-7138-4fe6-ac46-7c40879ddd25")
	)
	(pad "" smd roundrect
		(at 1.85 1.1)
		(size 1.4 2)
		(layers "F.Paste")
		(roundrect_rratio 0.1785714286)
		(uuid "23e722db-a579-4797-8a54-b7b1267141f4")
	)
	(pad "1" smd roundrect
		(at -1.85 0)
		(size 1.4 4.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.07142857143)
		(uuid "581a8ac7-0bf5-4fd3-b061-a06837e1d194")
	)
	(pad "2" smd roundrect
		(at 1.85 0)
		(size 1.4 4.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.07142857143)
		(uuid "f7ce2f27-3b85-48c2-ab95-43e048d58442")
	)
	(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Sunlord_SWPA5040S.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
