(footprint "Everlight_ITR9608-F"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Fork-type photointerrupter (https://everlighteurope.com/index.php?controller=attachment&id_attachment=5389)")
	(tags "Photointerrupter infrared LED")
	(property "Reference" "U1"
		(at -1 -3 0)
		(layer "F.SilkS")
		(uuid "72279618-3338-4422-8536-6f29e254287f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
			(justify right)
		)
	)
	(property "Value" "ITR9608-F"
		(at 5 5.77 0)
		(layer "F.Fab")
		(uuid "24491d74-0caa-4681-9fe6-a7deb4f6cfb5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "OptoDevice:Everlight_ITR9608-F"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "54b213db-2dcb-47f9-9f5b-ac7d35b85227")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" "https://everlighteurope.com/index.php?controller=attachment&id_attachment=5389"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0cdff678-e0e0-4899-b69d-92752a844c71")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" "Photointerrupter infrared LED with photo IC, -25 to +85 degree Celsius"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "029b16b5-54f8-4d56-b2bb-32e7d1f42b23")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "LCSC" "C52833"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "67dfadb3-3cd2-4b94-a0d8-30c107575506")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "ITR9608"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1c3412a2-d5c8-4098-920e-73ad57d535d6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "Everlight"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e1d643d1-ca7b-4339-8129-c6701605a4f2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -1.88 -2.11)
		(end -1.88 -0.23)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9604bbb7-f76b-4ed0-b670-c76a3601a979")
	)
	(fp_line
		(start -1.88 -2.11)
		(end 0 -2.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "79c66359-bf5b-4ee4-9197-411653c1d1e6")
	)
	(fp_line
		(start -1.62 -1.850001)
		(end 11.62 -1.85)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e9e78c1e-83ba-41f1-8ba7-fd30f56357ea")
	)
	(fp_line
		(start -1.62 4.39)
		(end -1.62 -1.850001)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2755e73c-204c-47fa-8a7d-4a348a3bad88")
	)
	(fp_line
		(start 1.3 0.77)
		(end 1.8 1.77)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "64071914-fe23-44de-9070-e660ba0c31d3")
	)
	(fp_line
		(start 1.8 0.77)
		(end 1.8 -0.23)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "199a475f-9290-4511-bf74-47be5e10644b")
	)
	(fp_line
		(start 1.8 1.77)
		(end 1.8 2.77)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0cc0b00e-15c6-45e1-96c8-47a0f1d86389")
	)
	(fp_line
		(start 1.8 1.77)
		(end 2.3 0.77)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4599785d-ee9f-446f-9ab0-4eb79c170032")
	)
	(fp_line
		(start 2.3 0.77)
		(end 1.3 0.77)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5ce7f213-0029-4ec1-9d35-796c59fb99f6")
	)
	(fp_line
		(start 2.300001 1.77)
		(end 1.3 1.77)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4952005a-d8d8-4cc5-8080-9a70fd99a462")
	)
	(fp_line
		(start 2.62 4.37)
		(end 2.62 -1.85)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5319d059-d6f6-4593-9a23-00c48195e316")
	)
	(fp_line
		(start 7.38 4.370001)
		(end 7.38 -1.850001)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9d62474d-010f-44cc-b115-6bb4a778053d")
	)
	(fp_line
		(start 11.62 -1.85)
		(end 11.62 4.39)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9bab15a3-a525-4b01-a3de-5ae9b77b23a0")
	)
	(fp_line
		(start 11.62 4.39)
		(end -1.62 4.39)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "74f4d71c-16fe-4ab0-8424-7deb06a51cd6")
	)
	(fp_circle
		(center 8.25 2.54)
		(end 8.55 2.54)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "f4593ac5-99ad-44a0-b28f-53278082a079")
	)
	(fp_line
		(start -1.75 4.52)
		(end -1.749999 -1.98)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b4717655-2ad0-4f02-8404-7219dc0448b8")
	)
	(fp_line
		(start -1.749999 -1.98)
		(end 11.75 -1.98)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "7a08ad19-9c5a-40e6-b4d3-41b56da9f74e")
	)
	(fp_line
		(start 11.75 -1.98)
		(end 11.75 4.52)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "bbd4368b-6726-4dea-885e-e5e67cb5343c")
	)
	(fp_line
		(start 11.75 4.52)
		(end -1.75 4.52)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ff321fa5-2c8c-4cc5-9c49-60229c607d74")
	)
	(fp_line
		(start -1.5 -0.73)
		(end -0.5 -1.73)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7cf3db48-d7d1-444e-bdf5-bfaf55675faf")
	)
	(fp_line
		(start -1.5 4.27)
		(end -1.5 -0.73)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2e5499a3-f986-412a-9523-7d2f8b61f927")
	)
	(fp_line
		(start -0.5 -1.73)
		(end 11.5 -1.73)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "25861a21-f424-4542-9c27-29b2911e24cf")
	)
	(fp_line
		(start 1.3 0.77)
		(end 1.8 1.77)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "10fd57b1-2b21-4a1f-ad7d-40a574e5c871")
	)
	(fp_line
		(start 1.8 0.77)
		(end 1.8 -0.23)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "00e347a9-84b1-4ae6-9c80-68a65d337ba5")
	)
	(fp_line
		(start 1.8 1.77)
		(end 1.8 2.77)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b54f0dc5-f7f3-4b66-9943-fe8b9b1070cf")
	)
	(fp_line
		(start 1.8 1.77)
		(end 2.3 0.77)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2fde957c-a443-4899-b698-add56517c2c9")
	)
	(fp_line
		(start 2.3 0.77)
		(end 1.3 0.77)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7498b1ad-5ad4-4fad-b03d-a484b58e89d8")
	)
	(fp_line
		(start 2.300001 1.77)
		(end 1.3 1.77)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "20666b38-5e51-46f8-910b-000e176ab351")
	)
	(fp_line
		(start 2.5 -1.73)
		(end 2.5 4.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "29a2936e-8d79-4b4f-bac0-fa1b155e87f5")
	)
	(fp_line
		(start 7.5 -1.73)
		(end 7.5 4.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e095a074-0f7a-4edc-af76-b7938b86322c")
	)
	(fp_line
		(start 11.5 -1.73)
		(end 11.5 4.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "cf6cca7d-6f8e-4b71-9a6d-d95ca2540abc")
	)
	(fp_line
		(start 11.5 4.27)
		(end -1.5 4.27)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8a8c6095-1fd2-43cb-9bb5-16de566d8162")
	)
	(fp_text user "${REFERENCE}"
		(at 5 1.270001 0)
		(layer "F.Fab")
		(uuid "5754e2ce-f03a-4db0-b8cc-c8ac9f0a25d5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole roundrect
		(at 0 0 90)
		(size 1.5 2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.227)
		(uuid "c0de3e35-f190-48eb-a758-3708b66c084d")
	)
	(pad "2" thru_hole oval
		(at 0 2.54 90)
		(size 1.5 2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "51e2f057-dee4-4e0d-a28c-505e1342c896")
	)
	(pad "3" thru_hole oval
		(at 10 2.54 90)
		(size 1.5 2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "f222c314-b895-408b-ad85-704d3d2a3777")
	)
	(pad "4" thru_hole oval
		(at 10 0 90)
		(size 1.5 2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1a6d4598-a11b-456f-b164-f29b1fb396cf")
	)
	(model "${KICAD6_3DMODEL_DIR}/OptoDevice.3dshapes/Everlight_ITR9608-F.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "/home/stefan/kicad/library/3dmodels/Sensor_Optical.3dshapes/Everlight ITR9608.step"
		(offset
			(xyz 5 -1.27 6.8)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)