(module Micro_5P (layer F.Cu) (tedit 57DFE117)
  (attr virtual)
  (fp_text reference J1 (at -3.1 0) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value CONN (at 0 -1.3) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (pad 1 thru_hole roundrect (at -1.4 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)(roundrect_rratio 0.25))
  (pad 2 thru_hole roundrect (at -0.9 1.4) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)(roundrect_rratio 0.25))
  (pad 3 thru_hole roundrect (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)(roundrect_rratio 0.25))
  (pad 4 thru_hole roundrect (at 0.9 1.4) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)(roundrect_rratio 0.25))
  (pad 5 thru_hole roundrect (at 1.4 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)(roundrect_rratio 0.25))
)
