(footprint "Texas_VQFN-RHL-20"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "http://www.ti.com/lit/ds/symlink/bq51050b.pdf")
	(tags "RHL0020A")
	(property "Reference" "U11"
		(at 0 -3.5 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "33c4ad2b-93b0-40aa-85fb-a4aae1c09818")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "TXS0108ERGYR"
		(at 0 3.7 0)
		(layer "F.Fab")
		(uuid "b4ea77c9-e127-41c9-8085-706552d898f5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Package_DFN_QFN:Texas_VQFN-RHL-20"
		(at 0 0 180)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
		(uuid "22a9f7a4-22d9-4557-bec6-68f43b45853c")
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify mirror)
		)
	)
	(property "Datasheet" "www.ti.com/lit/ds/symlink/txs0108e.pdf"
		(at 0 0 180)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
		(uuid "56033313-ffe7-460f-b005-26321dff4f45")
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify mirror)
		)
	)
	(property "Description" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
		(uuid "28113f52-c825-4b4d-9129-e5c6b2bd1bb3")
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify mirror)
		)
	)
	(property "LCSC" "C90706"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "a1d9c227-0443-48e0-bf3d-db539556a3cb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "TI"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "85abe234-bdb5-4497-94bc-43b5be2be73d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "TXS0108ERGYR"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "01d22fef-f285-44a0-8c6f-2b6b6135ecea")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.8 2.3)
		(end -1.8 2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0f313b49-4f1a-4c7b-a347-7a792262c740")
	)
	(fp_line
		(start -1 -2.3)
		(end -1.9 -2.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "dc53735d-eb28-42d1-a03d-b14fc91e6455")
	)
	(fp_line
		(start -1 2.3)
		(end -1.8 2.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "206614ea-bba1-40b8-83c1-e8627aa88c35")
	)
	(fp_line
		(start 1.8 -2.3)
		(end 1 -2.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3cbb6ea4-42fe-42ee-9e2a-332881cb9cd2")
	)
	(fp_line
		(start 1.8 -2)
		(end 1.8 -2.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "80ca1220-8742-42db-b897-a9a9c8a0f738")
	)
	(fp_line
		(start 1.8 2.3)
		(end 1 2.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6812a5bc-0b94-4b6e-b638-c0e7a39f6ffd")
	)
	(fp_line
		(start 1.8 2.3)
		(end 1.8 2)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "43e64d1a-553a-4877-ac1e-3d503e8c5b2f")
	)
	(fp_line
		(start -2.1 -1.825)
		(end -2.1 1.825)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9e74d5b3-ea37-44bc-be4e-b78e92112292")
	)
	(fp_line
		(start -1.999228 -1.998649)
		(end -2 -2.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "178d613f-35fe-42a3-9238-cf1b3a35c70a")
	)
	(fp_line
		(start -1.999228 1.998649)
		(end -2 2.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "aeb44cd2-9e90-4fb9-921c-da357d396fcc")
	)
	(fp_line
		(start -0.998649 -2.499228)
		(end -1.75 -2.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "17d06a9c-40da-4168-89ed-8ef764402803")
	)
	(fp_line
		(start -0.998649 2.499228)
		(end -1.75 2.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "d968e2f6-7fc0-43d3-899a-d95df4a8dede")
	)
	(fp_line
		(start -0.825 2.6)
		(end 0.825 2.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "bed5a5d1-8513-468e-9570-f8e140cb8e6d")
	)
	(fp_line
		(start 0.825 -2.6)
		(end -0.825 -2.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "cb33fbb4-896c-4b4e-8e01-f94b5948a43d")
	)
	(fp_line
		(start 0.998649 -2.499228)
		(end 1.75 -2.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "cbe2c476-978c-4f9a-bcf0-a7131666daad")
	)
	(fp_line
		(start 0.998649 2.499228)
		(end 1.75 2.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "1c5f8a4d-0d2f-45b5-9c2e-8c2e53608fd9")
	)
	(fp_line
		(start 1.999228 -1.998649)
		(end 2 -2.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "075adcba-7f66-46b7-afaa-fb9d1c069211")
	)
	(fp_line
		(start 1.999228 1.998649)
		(end 2 2.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9706a6b1-b106-42a4-8c2a-485a8aeafe16")
	)
	(fp_line
		(start 2.1 1.825)
		(end 2.1 -1.825)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9dd4c74a-f287-401f-aa5d-9e7bdf80e136")
	)
	(fp_arc
		(start -2.1 -1.825)
		(mid -2.072982 -1.925385)
		(end -1.999228 -1.998649)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "2716eec6-a540-4f1b-ab14-5c24246a977d")
	)
	(fp_arc
		(start -2 -2.25)
		(mid -1.926777 -2.426777)
		(end -1.75 -2.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "b2c448a5-fee4-4341-aca2-96c07a53b267")
	)
	(fp_arc
		(start -1.999228 1.998649)
		(mid -2.072982 1.925385)
		(end -2.1 1.825)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "a971e2d7-6df9-4ead-8f75-2df0e67211cc")
	)
	(fp_arc
		(start -1.75 2.5)
		(mid -1.926777 2.426777)
		(end -2 2.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "be0bdf30-f9a6-4955-bf97-f3a799b4c9e8")
	)
	(fp_arc
		(start -0.998649 -2.499228)
		(mid -0.925385 -2.572982)
		(end -0.825 -2.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "1fbe5e92-868d-4be2-8d7f-4ca3f809253d")
	)
	(fp_arc
		(start -0.825 2.6)
		(mid -0.925385 2.572982)
		(end -0.998649 2.499228)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "2d2d440f-cd5f-4794-a6bb-b1068985af31")
	)
	(fp_arc
		(start 0.825 -2.6)
		(mid 0.925385 -2.572982)
		(end 0.998649 -2.499228)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "b6c8c116-7354-4421-9bb8-c479ab99cc7e")
	)
	(fp_arc
		(start 0.998649 2.499228)
		(mid 0.925386 2.572982)
		(end 0.825 2.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e68e440f-5902-428d-8921-10f75f7a7782")
	)
	(fp_arc
		(start 1.75 -2.5)
		(mid 1.926777 -2.426777)
		(end 2 -2.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "0c74b082-2f8e-4b1e-9d3f-8dc5986b0156")
	)
	(fp_arc
		(start 1.999228 -1.998649)
		(mid 2.072982 -1.925386)
		(end 2.1 -1.825)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5ce5df29-49d3-4756-be54-26fec6dfc0d2")
	)
	(fp_arc
		(start 2 2.25)
		(mid 1.926777 2.426777)
		(end 1.75 2.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "78e0b683-f882-4ceb-8fb5-ce4e6282ce67")
	)
	(fp_arc
		(start 2.1 1.825)
		(mid 2.072982 1.925385)
		(end 1.999228 1.998649)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "a63a7b15-e306-4e37-a9f9-6239eadd55d5")
	)
	(fp_line
		(start -1.75 2.25)
		(end -1.75 -2.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2003ae55-e780-4d70-877c-73fb9afe8031")
	)
	(fp_line
		(start -1.23 -2.25)
		(end -1.75 -1.73)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a6c681d7-62f5-4201-86cd-da72c961570e")
	)
	(fp_line
		(start 1.75 -2.25)
		(end -1.75 -2.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "03f537ae-45c0-4243-9de0-d259adb9449c")
	)
	(fp_line
		(start 1.75 2.25)
		(end -1.75 2.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "44f392c5-5dd7-4593-b806-93a89d31238a")
	)
	(fp_line
		(start 1.75 2.25)
		(end 1.75 -2.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2f9151ed-ab1e-4b17-af23-d2dec1bf59eb")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -3.5 0)
		(layer "F.Fab")
		(uuid "b70941ee-71d5-4f72-b720-59e2ed866369")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" smd oval
		(at -1.65 -1.75)
		(size 0.5 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "998655ac-8667-4256-b9e3-5978e2921369")
	)
	(pad "" smd oval
		(at -1.65 -1.25)
		(size 0.5 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "bf42d937-7ecd-49d4-a08b-7674eef0b22f")
	)
	(pad "" smd oval
		(at -1.65 -0.75)
		(size 0.5 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "f1fe390e-10be-4e13-b144-f176440b3a8e")
	)
	(pad "" smd oval
		(at -1.65 -0.25)
		(size 0.5 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "41a255fc-59b3-4caf-ae56-f9e3a45cd619")
	)
	(pad "" smd oval
		(at -1.65 0.25)
		(size 0.5 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "3bd14e7b-e524-4af1-b270-98c4b176cf73")
	)
	(pad "" smd oval
		(at -1.65 0.75)
		(size 0.5 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "719b8aa6-51de-4f80-bc31-10545f408d09")
	)
	(pad "" smd oval
		(at -1.65 1.25)
		(size 0.5 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "29eb3219-0810-4bf4-96e9-7ffd0219c4c7")
	)
	(pad "" smd oval
		(at -1.65 1.75)
		(size 0.5 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "fb2df2cb-19d3-483b-b6da-41120be6b25f")
	)
	(pad "" smd oval
		(at -0.75 -2.15 90)
		(size 0.5 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "ed1d64f0-7acc-4944-b093-4397c6f943ed")
	)
	(pad "" smd oval
		(at -0.75 2.15 90)
		(size 0.5 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "2468040f-ffc2-40a0-a666-d26ab2f585d9")
	)
	(pad "" smd roundrect
		(at -0.56 -1.05)
		(size 0.92 0.85)
		(layers "F.Paste")
		(roundrect_rratio 0.2352941176)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "75311e31-c66e-40ff-88e1-380c703bfc39")
	)
	(pad "" smd roundrect
		(at -0.56 0)
		(size 0.92 0.85)
		(layers "F.Paste")
		(roundrect_rratio 0.2352941176)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "a712a92c-3388-40fc-af15-9de4d6d165e9")
	)
	(pad "" smd roundrect
		(at -0.56 1.05)
		(size 0.92 0.85)
		(layers "F.Paste")
		(roundrect_rratio 0.2352941176)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "bcd1f1f2-847d-4d76-a894-114a8af25dbf")
	)
	(pad "" smd oval
		(at -0.275 -2.0125 90)
		(size 0.775 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "4cee381a-37fc-4b53-8f99-59e44288ec25")
	)
	(pad "" smd oval
		(at -0.275 2 90)
		(size 0.775 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "0fc5232a-e895-4d23-bea5-729bd85b32c4")
	)
	(pad "" smd oval
		(at 0.275 -2.0125 90)
		(size 0.775 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "ff6cc4f4-6426-439d-af84-f77ad1e0ea66")
	)
	(pad "" smd oval
		(at 0.275 2 90)
		(size 0.775 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "94dd0f2a-1dc8-4412-81ac-1c4bf237709e")
	)
	(pad "" smd roundrect
		(at 0.56 -1.05)
		(size 0.92 0.85)
		(layers "F.Paste")
		(roundrect_rratio 0.2352941176)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "9755c495-c391-4090-af1a-227b22743305")
	)
	(pad "" smd roundrect
		(at 0.56 0)
		(size 0.92 0.85)
		(layers "F.Paste")
		(roundrect_rratio 0.2352941176)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "ad773014-260a-41a3-9d9a-82bb2364df70")
	)
	(pad "" smd roundrect
		(at 0.56 1.05)
		(size 0.92 0.85)
		(layers "F.Paste")
		(roundrect_rratio 0.2352941176)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "7216035c-44a9-450c-ae7e-52023dbd0421")
	)
	(pad "" smd oval
		(at 0.75 -2.15 90)
		(size 0.5 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "05e6dff9-2c69-4821-bd3f-59b46ef517e7")
	)
	(pad "" smd oval
		(at 0.75 2.15 90)
		(size 0.5 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "f4af63a4-6906-44ca-a402-d62f1726c850")
	)
	(pad "" smd oval
		(at 1.65 -1.75)
		(size 0.5 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "e2810dbb-5067-41f8-9960-14af9066f4c3")
	)
	(pad "" smd oval
		(at 1.65 -1.25)
		(size 0.5 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "72306dae-4fa9-4b6a-aee3-3bddc824fd02")
	)
	(pad "" smd oval
		(at 1.65 -0.75)
		(size 0.5 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "b04ec5ff-d0eb-413c-9100-564a125704b7")
	)
	(pad "" smd oval
		(at 1.65 -0.25)
		(size 0.5 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "e37004c8-3052-46df-83cc-053253253e27")
	)
	(pad "" smd oval
		(at 1.65 0.25)
		(size 0.5 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "3867df16-a642-4c94-aa27-86909ba4044c")
	)
	(pad "" smd oval
		(at 1.65 0.75)
		(size 0.5 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "e2eb7add-6a37-47b1-b35f-703df90c45c6")
	)
	(pad "" smd oval
		(at 1.65 1.25)
		(size 0.5 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "d6d1668d-0937-45c7-afcb-ca398cb0a930")
	)
	(pad "" smd oval
		(at 1.65 1.75)
		(size 0.5 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "fe653c8c-5506-4c44-8821-dbc459d5e064")
	)
	(pad "1" smd roundrect
		(at -0.75 -2.15)
		(size 0.24 0.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.21)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "09dc189b-1d23-4be6-a8d6-2e4c46da697a")
	)
	(pad "2" smd roundrect
		(at -1.65 -1.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.21)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "e97d2aca-36be-4330-b6bd-60a05b7aab2d")
	)
	(pad "3" smd roundrect
		(at -1.65 -1.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.21)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "be7a5d25-9196-4a1d-9e00-d518a4c5c3bd")
	)
	(pad "4" smd roundrect
		(at -1.65 -0.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.21)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "13f64b6f-80b0-4dff-8bf6-3256646744d3")
	)
	(pad "5" smd roundrect
		(at -1.65 -0.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.21)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "fa68d498-e598-43a2-8d44-ef61bdab6548")
	)
	(pad "6" smd roundrect
		(at -1.65 0.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.21)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "657ce2de-9eb7-4e13-be1e-22df78174ba8")
	)
	(pad "7" smd roundrect
		(at -1.65 0.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.21)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "ccf6bd70-fb2a-4a0c-8cda-46e28cc35eac")
	)
	(pad "8" smd roundrect
		(at -1.65 1.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.21)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "0dc1e853-645a-41f0-b858-29d1c2ee4eed")
	)
	(pad "9" smd roundrect
		(at -1.65 1.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.21)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "ef560f97-7570-45f9-8974-ef406ea13617")
	)
	(pad "10" smd roundrect
		(at -0.75 2.15)
		(size 0.24 0.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.21)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "279dbc56-dde4-4ad9-a3c9-c5feffbf7e04")
	)
	(pad "11" smd roundrect
		(at 0.75 2.15)
		(size 0.24 0.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.21)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "344596e5-ff43-4e46-90e3-7e3681473708")
	)
	(pad "12" smd roundrect
		(at 1.65 1.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.21)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "497e8048-7e4a-45bb-aafa-57ebcbf8eaf0")
	)
	(pad "13" smd roundrect
		(at 1.65 1.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.21)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "8ffc50c5-7982-4a95-9a6a-e2e4aa8d703f")
	)
	(pad "14" smd roundrect
		(at 1.65 0.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.21)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "6561c8dc-e56b-45a8-a255-4c12bdc1a93f")
	)
	(pad "15" smd roundrect
		(at 1.65 0.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.21)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "554a0fed-24d5-455b-a016-76a77679c24f")
	)
	(pad "16" smd roundrect
		(at 1.65 -0.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.21)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "c2d7160a-d0b8-40fa-82d4-e7378bdf678a")
	)
	(pad "17" smd roundrect
		(at 1.65 -0.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.21)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "516e2fd5-20d9-4ca5-a71e-2e1ce2f03b7f")
	)
	(pad "18" smd roundrect
		(at 1.65 -1.25)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.21)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "33f023d2-70dc-4249-bbcb-735a4ff26c2c")
	)
	(pad "19" smd roundrect
		(at 1.65 -1.75)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.21)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "d89c8378-8524-4c7f-b4a0-8973cb8ff492")
	)
	(pad "20" smd roundrect
		(at 0.75 -2.15)
		(size 0.24 0.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.21)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "fe037028-b69d-4f52-b62a-0bea449d72ce")
	)
	(pad "21" smd roundrect
		(at -0.275 -2.15)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
		(zone_connect 2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "61f5316c-4b41-4271-8e02-782a5f0b0e82")
	)
	(pad "21" smd roundrect
		(at -0.275 2.15)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
		(zone_connect 2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "b3b110a7-83bd-4324-ba13-05ce7c1da3e6")
	)
	(pad "21" smd custom
		(at 0 0)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.375 -1.525) (xy 1.025 -1.525) (xy 1.025 1.525) (xy 0.375 1.525) (xy 0.375 1.925) (xy -0.375 1.925)
					(xy -0.375 1.525) (xy -1.025 1.525) (xy -1.025 -1.525) (xy -0.375 -1.525) (xy -0.375 -1.925) (xy 0.375 -1.925)
				)
				(width 0)
				(fill yes)
			)
		)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "305d292c-15f4-4cb2-9fa5-ab3529301424")
	)
	(pad "21" smd roundrect
		(at 0.275 -2.15)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
		(zone_connect 2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1f1a9291-d698-4432-8eb2-ff71fc639aaf")
	)
	(pad "21" smd roundrect
		(at 0.275 2.15)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
		(zone_connect 2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "c2120e70-36a2-4fe0-a640-6abba0cd48cd")
	)
	(model ":KICAD7_3DMODEL_DIR:Package_DFN_QFN.3dshapes/Texas_RGY_R-PVQFN-N20_EP2.05x3.05mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)