(footprint "USB_C_Receptacle_XKB_U264-141N-4BAC10"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "J21"
		(at -2.25 2.95 90)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "538c78d5-f261-44c9-8781-f4a217a155b2")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "USB-C 2.0 0"
		(at 0 -7.3 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "3f7c9924-c24c-4bec-9aef-d4ef220190e1")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.0625)
			)
		)
	)
	(property "Footprint" "Connector_USB:USB_C_Receptacle_XKB_U264-141N-4BAC10"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b0423d3b-e4e9-4f1e-85ed-2a7f7dafb64c")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b15b0045-8ee0-4d64-816f-965f6bf4638e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "aaa0560a-8145-4ded-b643-1efc05ba0dd6")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C692526"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "0e57dadc-bb6f-4073-8666-b46a8b3d63f2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "XKB"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "92fcf840-c405-40e7-927d-08051fc7e0e3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "U264-141N-4BAC10"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
		(uuid "d402ce8f-6ae4-4520-93f0-7618eb1557c4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -1.58 4.85)
		(end -1.58 1)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c6ec12e3-61b7-4e5d-b7c1-b4ac68de6c48")
	)
	(fp_line
		(start -0.75 7)
		(end 0.75 7)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "3c33ac52-b782-46bc-a27b-bf4e70e0ba46")
	)
	(fp_line
		(start 1.58 4.85)
		(end 1.58 1)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "32621558-5c8a-4ffc-b211-608dcc0947cb")
	)
	(fp_line
		(start -2.025 -0.65)
		(end -2.025 0.65)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "cfc9bb15-e7e0-4a21-ac80-899062dbf806")
	)
	(fp_line
		(start -2.025 5.2)
		(end -2.025 7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "ccd3c6c3-c0c8-4759-af47-87111e7fa59d")
	)
	(fp_line
		(start -1.725 -0.95)
		(end -1.125 -0.95)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "b148ba0c-4e82-4f9a-a289-ebf67db35126")
	)
	(fp_line
		(start -1.725 0.95)
		(end -0.825 0.95)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "1b355613-87bf-47b6-b0dd-09fb5fe1c85f")
	)
	(fp_line
		(start -1.725 7.3)
		(end -1.125 7.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "2f65eafa-2df2-47ea-bb5b-13251ddbaa9a")
	)
	(fp_line
		(start -0.825 -0.475)
		(end -0.825 -0.65)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "71cba951-946d-46aa-a870-23238eb8c8a2")
	)
	(fp_line
		(start -0.825 0.95)
		(end -0.825 4.9)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "9a40b9cb-ef77-4572-8178-b8cc25771711")
	)
	(fp_line
		(start -0.825 4.9)
		(end -1.725 4.9)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "0d29af0a-2303-4c4f-9823-a6d458c3e122")
	)
	(fp_line
		(start -0.825 6.425)
		(end -0.825 7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "e019f01f-a085-488f-b927-8164adf9cfd3")
	)
	(fp_line
		(start 0.825 -0.475)
		(end -0.825 -0.475)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "40b27629-c438-4a3b-bfde-5f9f56c9129c")
	)
	(fp_line
		(start 0.825 -0.475)
		(end 0.825 -0.65)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "138aa7f0-8c86-46bf-844b-ddeecc9afd7f")
	)
	(fp_line
		(start 0.825 0.95)
		(end 0.825 4.9)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "1024e4a1-e359-4ee4-aacc-213b9195604f")
	)
	(fp_line
		(start 0.825 4.9)
		(end 1.725 4.9)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "3663e181-6300-4e01-b30e-924c3c32fa57")
	)
	(fp_line
		(start 0.825 6.425)
		(end -0.825 6.425)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "7f8ee09d-a95a-48c1-8003-e1de82a94f73")
	)
	(fp_line
		(start 0.825 6.425)
		(end 0.825 7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "6ff27f4c-7976-4820-ad72-53e11248a37e")
	)
	(fp_line
		(start 1.725 -0.95)
		(end 1.125 -0.95)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "f5406400-a6af-403b-b826-dba915f93daf")
	)
	(fp_line
		(start 1.725 0.95)
		(end 0.825 0.95)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "40309a37-7245-4a9a-a0c1-2a1364e92294")
	)
	(fp_line
		(start 1.725 7.3)
		(end 1.125 7.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "3bc7404b-1c9c-449a-a4e2-aaa9e0afdd3f")
	)
	(fp_line
		(start 2.025 -0.65)
		(end 2.025 0.65)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "858fc1cf-3589-48be-9df5-afef0b84a74a")
	)
	(fp_line
		(start 2.025 5.2)
		(end 2.025 7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "733fc8c8-0435-446b-b55e-d9c41dfb00ff")
	)
	(fp_arc
		(start -2.025 -0.65)
		(mid -1.937132 -0.862132)
		(end -1.725 -0.95)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "69c3eed6-004b-434c-aa4d-c8a04fb0c860")
	)
	(fp_arc
		(start -2.025 5.2)
		(mid -1.937132 4.987868)
		(end -1.725 4.9)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "273534fe-e40e-4974-b396-4abd12734d9f")
	)
	(fp_arc
		(start -1.725 0.95)
		(mid -1.937132 0.862132)
		(end -2.025 0.65)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "92a9df07-8d84-44da-8c1d-96a06036a03b")
	)
	(fp_arc
		(start -1.725 7.3)
		(mid -1.937132 7.212132)
		(end -2.025 7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "b76006d4-da04-44be-9576-650bf4fee27b")
	)
	(fp_arc
		(start -1.125 -0.95)
		(mid -0.912868 -0.862132)
		(end -0.825 -0.65)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "dc19945c-0e5e-467b-b24f-c516c0d7d737")
	)
	(fp_arc
		(start -0.825 7)
		(mid -0.912868 7.212132)
		(end -1.125 7.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "aceab4f7-9a5d-45a2-a30d-3f5fa84c4221")
	)
	(fp_arc
		(start 0.825 -0.65)
		(mid 0.912868 -0.862132)
		(end 1.125 -0.95)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "fc2415a1-cf8b-4541-8976-6e81e9f48bcc")
	)
	(fp_arc
		(start 1.125 7.3)
		(mid 0.912868 7.212132)
		(end 0.825 7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "0b2c5830-54e6-4291-84be-e152ed884ddf")
	)
	(fp_arc
		(start 1.725 -0.95)
		(mid 1.937132 -0.862132)
		(end 2.025 -0.65)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "5b745a81-1234-464e-b2f7-ce9c2b922c4c")
	)
	(fp_arc
		(start 1.725 4.9)
		(mid 1.937132 4.987868)
		(end 2.025 5.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "7f4c1f9c-3c16-4b16-bf38-ba47ba968276")
	)
	(fp_arc
		(start 2.025 0.65)
		(mid 1.937132 0.862132)
		(end 1.725 0.95)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "4fac8910-5100-495c-8d17-e33aa6ad52ae")
	)
	(fp_arc
		(start 2.025 7)
		(mid 1.937132 7.212132)
		(end 1.725 7.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "B.CrtYd")
		(uuid "dbb63fb4-f248-4860-bff0-3c338d117534")
	)
	(fp_line
		(start -2.05 -0.65)
		(end -2.05 7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "2405762e-eddc-4a31-8cce-dec060e705ab")
	)
	(fp_line
		(start -1.75 7.3)
		(end 1.75 7.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "daf8a64d-1ea0-4a13-800e-c1b59daa2fdd")
	)
	(fp_line
		(start 1.75 -0.95)
		(end -1.75 -0.95)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f319cc86-4b14-4341-8f12-86b1db9a67ef")
	)
	(fp_line
		(start 2.05 7)
		(end 2.05 -0.65)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "8d22e355-a27f-4c86-9715-d7bbcda007a0")
	)
	(fp_arc
		(start -2.05 -0.65)
		(mid -1.962132 -0.862132)
		(end -1.75 -0.95)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "3d4b5f68-d6c0-4dab-9c89-70b24353f2c0")
	)
	(fp_arc
		(start -1.75 7.3)
		(mid -1.962132 7.212132)
		(end -2.05 7)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "3cc1e6e1-b168-4b6f-a3b4-e10a6a7f835e")
	)
	(fp_arc
		(start 1.75 -0.95)
		(mid 1.962132 -0.862132)
		(end 2.05 -0.65)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "be9780a0-2c73-49f4-9d94-b403e8397e36")
	)
	(fp_arc
		(start 2.05 7)
		(mid 1.962132 7.212132)
		(end 1.75 7.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "1eddd7d5-9262-4bd7-a861-b2e0114356b4")
	)
	(fp_rect
		(start -1.83 -7)
		(end 1.83 7)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "052051d3-3a64-4208-ab51-d31e6e2ea957")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -6.7 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "11b130e9-eccd-4257-9276-12e85e81f4f9")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.0625)
			)
		)
	)
	(pad "A1" thru_hole circle
		(at 0.375 0.05)
		(size 0.6 0.6)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "30ce428d-4a17-447d-bc0b-3cef85072e77")
	)
	(pad "A1" connect roundrect
		(at 0.375 0.05)
		(size 0.6 0.75)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "5d7fc788-0b15-4b2f-960f-21323f997ea8")
	)
	(pad "A4" thru_hole circle
		(at 0.375 0.95)
		(size 0.6 0.6)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "a495dc8b-28d1-4eba-a6bd-c2f44e9229e4")
	)
	(pad "A4" connect roundrect
		(at 0.375 0.95)
		(size 0.6 0.75)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "3f6a5378-13b5-4533-8f1c-656b3b74522f")
	)
	(pad "A5" thru_hole circle
		(at 0.375 1.85)
		(size 0.6 0.6)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "70a0e0f5-80e3-4d5d-bdf4-900bc0b790b5")
	)
	(pad "A5" connect roundrect
		(at 0.375 1.85)
		(size 0.6 0.75)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "7f25dabc-4d74-4b66-80e0-54bc37690a1a")
	)
	(pad "A6" thru_hole circle
		(at 0.375 2.75)
		(size 0.6 0.6)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "81aa8e54-0877-4c6b-93cf-750f21361e26")
	)
	(pad "A6" connect roundrect
		(at 0.375 2.75)
		(size 0.6 0.75)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "cc9d52fb-5578-4717-9119-32a5d01e113d")
	)
	(pad "A7" thru_hole circle
		(at 0.375 3.65)
		(size 0.6 0.6)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "2f9d94d7-78c2-4dcd-afc0-07c72a02680a")
	)
	(pad "A7" connect roundrect
		(at 0.375 3.65)
		(size 0.6 0.75)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "2b77fa0b-783d-41aa-a3c7-dfe50ece7652")
	)
	(pad "A9" thru_hole circle
		(at 0.375 5)
		(size 0.6 0.6)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "8686f6a7-78b1-49b0-a540-b17c1d1e2b7f")
	)
	(pad "A9" connect roundrect
		(at 0.375 5)
		(size 0.6 0.75)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "a621726f-cd06-4d9b-8d72-8b84925411b1")
	)
	(pad "A12" thru_hole circle
		(at 0.375 5.9)
		(size 0.6 0.6)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1cdb2dc8-38b4-4127-bba3-9c34da119e5a")
	)
	(pad "A12" connect roundrect
		(at 0.375 5.9)
		(size 0.6 0.75)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "dd7abbb1-e730-4bf4-be76-48b74d1f10cf")
	)
	(pad "B1" thru_hole circle
		(at -0.375 5.9)
		(size 0.6 0.6)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "125046dd-01af-423a-baa6-87e8520b6159")
	)
	(pad "B1" connect roundrect
		(at -0.375 5.9)
		(size 0.6 0.75)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "b35baa33-03ae-41b1-a624-b6852abc0c0c")
	)
	(pad "B4" thru_hole circle
		(at -0.375 5)
		(size 0.6 0.6)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "ec98c8ec-da0b-49f2-a595-fb3dcaaace06")
	)
	(pad "B4" connect roundrect
		(at -0.375 5)
		(size 0.6 0.75)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "41bbab33-d04c-471a-a4c0-c380abc4a980")
	)
	(pad "B5" thru_hole circle
		(at -0.375 4.1)
		(size 0.6 0.6)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "8e0d2f6a-72fe-4679-9689-99ad96a73970")
	)
	(pad "B5" connect roundrect
		(at -0.375 4.1)
		(size 0.6 0.75)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "4acda5bf-00e1-449d-84aa-c949bcb0bd86")
	)
	(pad "B6" thru_hole circle
		(at -0.375 3.2)
		(size 0.6 0.6)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "035a59e5-0f73-413a-9dd3-192a24acfd90")
	)
	(pad "B6" connect roundrect
		(at -0.375 3.2)
		(size 0.6 0.75)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "3c06febd-f377-4902-849f-60334930c5c3")
	)
	(pad "B7" thru_hole circle
		(at -0.375 2.3)
		(size 0.6 0.6)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "ce68512f-ea89-41bc-8f31-e6d4fa758ed2")
	)
	(pad "B7" connect roundrect
		(at -0.375 2.3)
		(size 0.6 0.75)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "58edf545-b541-4f8a-8416-ddefeeb36fa1")
	)
	(pad "B9" thru_hole circle
		(at -0.375 0.95)
		(size 0.6 0.6)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "14503ae3-2da0-48da-b180-aa09995ff8ee")
	)
	(pad "B9" connect roundrect
		(at -0.375 0.95)
		(size 0.6 0.75)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "14980a5a-9826-40c2-9298-ea941e82de90")
	)
	(pad "B12" thru_hole circle
		(at -0.375 0.05)
		(size 0.6 0.6)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "49225a16-7716-441a-9045-778945a2a8ae")
	)
	(pad "B12" connect roundrect
		(at -0.375 0.05)
		(size 0.6 0.75)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.25)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "31d13cf9-c6cd-4e87-ae38-f4205501a2cd")
	)
	(pad "S1" thru_hole oval
		(at -1.43 0)
		(size 0.7 1.4)
		(drill oval 0.5 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "8734cd2d-f37e-412a-a479-9da24b51f24b")
	)
	(pad "S1" connect roundrect
		(at -1.43 0)
		(size 0.9 1.6)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.1666666667)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "5abeb7b8-64b1-40eb-9bf6-e779552064f2")
	)
	(pad "S1" thru_hole oval
		(at -1.43 6.1)
		(size 0.7 1.9)
		(drill oval 0.5 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "55cb4302-77dc-48a5-88e9-d132264f5b25")
	)
	(pad "S1" connect roundrect
		(at -1.43 6.1)
		(size 0.9 2.1)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.1666666667)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "77755949-ca61-49e7-8b4f-e720df2d2520")
	)
	(pad "S1" thru_hole oval
		(at 1.43 0)
		(size 0.7 1.4)
		(drill oval 0.5 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers yes)
		(keep_end_layers yes)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "563694cf-9ba3-4799-9fea-2b6d38476141")
	)
	(pad "S1" connect roundrect
		(at 1.43 0)
		(size 0.9 1.6)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.1666666667)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1f498d4b-7d0b-46fb-b577-6de44329ee46")
	)
	(pad "S1" thru_hole oval
		(at 1.43 6.1)
		(size 0.7 1.9)
		(drill oval 0.5 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "b58e53ec-404f-4a28-ab2f-0908497b534e")
	)
	(pad "S1" connect roundrect
		(at 1.43 6.1)
		(size 0.9 2.1)
		(layers "B.Cu" "B.Mask")
		(roundrect_rratio 0.1666666667)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.5)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled no)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "309b41f3-3778-4d0e-93b2-08caf72eb921")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(uuid "98218eac-7511-40ad-8ce9-4c3f29b5f0fd")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads not_allowed)
			(copperpour allowed)
			(footprints not_allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -2.05 -0.95) (xy 2.05 -0.95) (xy 2.05 -7.25) (xy -2.05 -7.25)
			)
		)
	)
	(model ":KICAD7_3DMODEL_DIR:Connector_USB.3dshapes/u264-14xn-4bac10.stp"
		(offset
			(xyz 0 7 9.05)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 90)
		)
	)
)
