(footprint "AMASS_XT60PW-M_1x02_P7.20mm_Horizontal" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Connector XT60 Horizontal PCB Female, https://www.tme.eu/en/Document/9b8d0c5eb7094295f3d3112c214d3ade/XT60PW%20SPEC.pdf")
  (tags "RC Connector XT60")
  (property "Sheetfile" "Servo_Controller.kicad_sch")
  (property "Sheetname" "")
  (property "ki_description" "Generic connectable mounting pin connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "connector")
  (attr through_hole)
  (fp_text reference "J3" (at 0 19.4 180) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3e1101f2-1467-4a79-b336-68fbd7fcbd15)
  )
  (fp_text value "VM" (at 0 17.15) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp df730d6d-9ca8-48b2-ad9e-bf417f9b955f)
  )
  (fp_text user "-" (at -3.6 19.15) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 455bf969-bb6e-4907-9b5d-b7f06c6e5163)
  )
  (fp_text user "+" (at 3.6 19.15) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9977df2d-4fd9-417d-8b35-24f2e2d6d9b9)
  )
  (fp_text user "${REFERENCE}" (at 0 12.75) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9fe14111-6840-4e8d-b586-6dfad15df98a)
  )
  (fp_line (start -7.85 -0.11) (end -7.85 14.45)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8a73a5f4-bc43-4b78-bd66-acd0258f9915))
  (fp_line (start -7.85 -0.11) (end 7.85 -0.1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4bcd6d11-954a-4052-92ab-0321fad2808e))
  (fp_line (start -6.056682 18.55721) (end 6.056682 18.55721)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3e41fb9a-8011-4efc-890a-8fded2a733e0))
  (fp_line (start 7.85 -0.1) (end 7.85 14.45)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 21b9888b-e00a-4dc1-a3de-b8378ade8288))
  (fp_arc (start -6.056682 18.55721) (mid -7.382125 16.690824) (end -7.85 14.45)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 1429d21b-9b71-41f8-ab7f-ea5d3ddec8f5))
  (fp_arc (start 7.85 14.45) (mid 7.382125 16.690824) (end 6.056682 18.55721)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp b4c2fdc2-393f-4b2a-9aa9-282c2bde570a))
  (fp_line (start -8.25 0) (end -8.25 14.45)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5002c844-2a76-49f2-90f7-ff95ca22f8b8))
  (fp_line (start -7.75 -0.5) (end 7.75 -0.5)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp dcb8f2ea-7cfa-4a51-b082-bba5ad831a95))
  (fp_line (start 6.236183 18.934456) (end -6.236183 18.934456)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cb89f95d-bc29-452c-a4d9-6673932aab75))
  (fp_line (start 8.25 0) (end 8.25 14.45)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3e659c44-9488-40c9-a182-4214b86e07ca))
  (fp_arc (start -8.25 0) (mid -8.103553 -0.353553) (end -7.75 -0.5)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 59163d50-e3e5-44ab-9237-fe96c7091cc8))
  (fp_arc (start -6.236183 18.934456) (mid -7.72344 16.907936) (end -8.25 14.45)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 6ca68bfd-fd44-4e3e-ad3c-2d98154f8ad7))
  (fp_arc (start 7.75 -0.5) (mid 8.103553 -0.353553) (end 8.25 0)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp b4557735-94e6-4c1b-a461-5b897efb7259))
  (fp_arc (start 8.25 14.45) (mid 7.72344 16.907936) (end 6.236183 18.934456)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 77240761-c557-4f82-a807-0e0c9d0f863a))
  (fp_line (start -7.75 0) (end -7.75 14.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8e17c57c-2e12-4234-a01b-7ac72047dcc4))
  (fp_line (start -7.75 0) (end 7.75 0)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 73ede193-ce51-42ca-a8ba-7b1f4734f9d1))
  (fp_line (start -6.038122 18.437497) (end 6.038122 18.437497)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp cdc7ca07-c3ba-4cdf-863f-1c7dc5db11f0))
  (fp_line (start 7.75 0) (end 7.75 14.45)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 42ddb76a-2589-4379-8a41-3eacc2bda639))
  (fp_arc (start -6.038122 18.437497) (mid -7.303943 16.619715) (end -7.75 14.45)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp 7735679d-f1d7-49cd-b42f-67ff431e8f4e))
  (fp_arc (start 7.75 14.45) (mid 7.303943 16.619715) (end 6.038122 18.437497)
    (stroke (width 0.1) (type default)) (layer "F.Fab") (tstamp d2c737a4-1864-4912-a75e-fd5468e474f7))
  (pad "1" thru_hole circle (at -3.6 16.35) (size 3 3) (drill 2.6) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (tstamp 52d0e5c6-e655-4325-9831-e9b420ecfdee))
  (pad "1" connect roundrect (at -3.6 16.35) (size 4.2 4.2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.119047619) (tstamp 9998b575-9cc3-46ed-932d-09f96e417013))
  (pad "2" thru_hole circle (at 3.6 16.35) (size 3 3) (drill 2.6) (layers "*.Cu" "*.Mask") (remove_unused_layers) (keep_end_layers) (tstamp 6eebd1b6-09db-468c-9141-a054565a88fc))
  (pad "2" connect roundrect (at 3.6 16.35) (size 4.2 4.2) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.3571428571) (tstamp a5077aea-a822-4eb7-b4cd-5a9de9f7301c))
  (pad "MP" thru_hole roundrect (at -6.75 10.35) (size 0.9 2) (drill oval 0.6 1.7) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.15625) (tstamp be30d007-09d5-430f-9269-b20e6a238885))
  (pad "MP" connect roundrect (at -6.75 10.35) (size 1.6 2.7) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.15625) (tstamp 4c528a04-9281-47cc-9683-3c0354e8b549))
  (pad "MP" thru_hole roundrect (at 6.75 10.35) (size 0.9 2) (drill oval 0.6 1.7) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.15625) (tstamp 77227106-4288-4688-bce2-0f59d38615eb))
  (pad "MP" connect roundrect (at 6.75 10.35) (size 1.6 2.7) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.15625) (tstamp efd8ce6b-3833-484b-b929-b56c2071c292))
  (model ":KICAD7_3DMODEL_DIR:Connector_AMASS.3dshapes/Amass XT60PW-M20.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
