(footprint "JST_SH_BM02B-SRSS-TB_1x02-1MP_P1.00mm_Vertical" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "JST SH series connector, BM02B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
  (tags "connector JST SH side entry")
  (property "Field2" "")
  (property "Sheetfile" "Flight Controller.kicad_sch")
  (property "Sheetname" "Flight Controller")
  (property "ki_description" "Generic connectable mounting pin connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
  (property "ki_keywords" "connector")
  (attr smd)
  (fp_text reference "J40" (at 0 -3.3) (layer "F.SilkS")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 82551a09-95d8-4371-bd6d-8367fa41da70)
  )
  (fp_text value "BAT" (at 0 3.3) (layer "F.Fab")
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 95531db2-a93e-41a9-b40a-aa48ca40ff59)
  )
  (fp_text user "${REFERENCE}" (at 0 -2.3) (layer "F.Fab")
      (effects (font (size 0.25 0.25) (thickness 0.0625)))
    (tstamp 5054f61f-1683-4c71-a9d6-18053733f59c)
  )
  (fp_rect (start -1 -2.1) (end 1 -1.95)
    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 03f8818b-5692-4ed5-a22d-d28a9ae9b583))
  (fp_arc (start -2.05 1.125) (mid -2.103033 1.103033) (end -2.125 1.05)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp d3275ec4-3ce7-4949-ae08-b1e0481e294e))
  (fp_arc (start -1.15 1.125) (mid -1.096967 1.146967) (end -1.075 1.2)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 8050da0f-0aed-42a3-8877-35eb7990f297))
  (fp_arc (start 2.125 1.05) (mid 2.103033 1.103033) (end 2.05 1.125)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 7c30e0d9-f156-49c7-a07e-0c8ea57c5c95))
  (fp_poly
    (pts
      (xy 2.05 0)
      (xy 2.2 0)
      (xy 2.2 1.05)
      (xy 2.05 1.2)
      (xy 1.05 1.2)
      (xy 1.05 1.05)
      (xy 2.05 1.05)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp bf5db68c-b1bf-45f8-8851-de4594dec415))
  (fp_poly
    (pts
      (xy -1.15 1.05)
      (xy -1 1.2)
      (xy -1 2.1)
      (xy -1.15 2.1)
      (xy -1.15 1.2)
      (xy -2.05 1.2)
      (xy -2.2 1.05)
      (xy -2.2 0.05)
      (xy -2.05 0.05)
      (xy -2.05 1.05)
    )

    (stroke (width 0) (type solid)) (fill solid) (layer "F.SilkS") (tstamp eac43780-88c1-447b-a047-9cc805930e10))
  (fp_line (start -2.55 -0.55) (end -2.55 -1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 929ee675-4640-4191-83cc-7701a3a07fa6))
  (fp_line (start -2.25 1) (end -2.249266 -0.161944)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 2deada75-4d85-48d4-ac8c-50f31f60c81c))
  (fp_line (start -2 1.25) (end -0.95 1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 32938c0e-8b33-487b-ab5e-5fa67ab8ec96))
  (fp_line (start -0.95 1.25) (end -0.95 1.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 406a0c6c-a384-48fb-81c4-9ce4d3a3a356))
  (fp_line (start 0.65 2.25) (end -0.65 2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 0723fe14-61d2-4b8b-aae8-8c4d24c2a423))
  (fp_line (start 0.95 1.25) (end 0.95 1.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 53994d50-1ddd-4f0c-bea6-0a75a85aaee6))
  (fp_line (start 2 1.25) (end 0.95 1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp dbe81163-08cd-4454-b579-dc1d48349c68))
  (fp_line (start 2.15 -2.25) (end -2.15 -2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 95ce0020-88f7-4e0e-b2c4-07f823abded7))
  (fp_line (start 2.25 1) (end 2.249266 -0.161944)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 39fa658e-e09c-4453-b902-3728ff1ceb1e))
  (fp_line (start 2.55 -0.55) (end 2.55 -1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fa226de6-8ed3-473e-b5d2-43f508bff07e))
  (fp_arc (start -2.55 -1.85) (mid -2.432843 -2.132843) (end -2.15 -2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d75eaf0c-8dc7-468f-b248-f92ce9839c9c))
  (fp_arc (start -2.249266 -0.161944) (mid -2.466016 -0.304527) (end -2.55 -0.55)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 86b87d1a-cb77-4981-ac5f-b69138d349a5))
  (fp_arc (start -2 1.25) (mid -2.176777 1.176777) (end -2.25 1)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 1bf473b1-58e7-4ba4-b6e7-9097c7c3f5e8))
  (fp_arc (start -0.65 2.25) (mid -0.862132 2.162132) (end -0.95 1.95)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp fa2263b1-eb22-420e-b42b-477e60611270))
  (fp_arc (start 0.95 1.95) (mid 0.862132 2.162132) (end 0.65 2.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d8db24fb-0cdd-4169-9906-596c37b9e6fb))
  (fp_arc (start 2.15 -2.25) (mid 2.432843 -2.132843) (end 2.55 -1.85)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp a67e5b71-0827-419e-8651-d1fee322b0fa))
  (fp_arc (start 2.25 1) (mid 2.176777 1.176777) (end 2 1.25)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp 80708a9f-dcbc-4b28-864c-82a18d0a398b))
  (fp_arc (start 2.55 -0.55) (mid 2.466016 -0.304527) (end 2.249266 -0.161944)
    (stroke (width 0.05) (type default)) (layer "F.CrtYd") (tstamp d66059c6-4ef9-4a96-9496-193763abc62d))
  (fp_line (start -2 -1.9) (end 2 -1.9)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0c6e324d-8a6d-4183-be4e-caba1b984a17))
  (fp_line (start -2 1) (end -2 -1.9)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp da95c0cc-4b46-433a-b5d9-babb8c02e26f))
  (fp_line (start -2 1) (end 2 1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 43336ad1-9726-4933-8de9-11a70ae7ed29))
  (fp_line (start -1 1) (end -0.5 0.292893)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bcb927f4-f8e9-4a2f-b787-cbac1d832a27))
  (fp_line (start -0.65 -1.55) (end -0.65 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 491943ed-1033-4253-b3e3-0ebc66c90198))
  (fp_line (start -0.65 -0.95) (end -0.35 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cc6206ff-66a0-4f25-856a-c5628e577e33))
  (fp_line (start -0.5 0.292893) (end 0 1)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f3588e52-2e8c-4dea-b1ef-e853d58e94f0))
  (fp_line (start -0.35 -1.55) (end -0.65 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a6e856eb-7aeb-4411-9046-89789a4f2234))
  (fp_line (start -0.35 -0.95) (end -0.35 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp babdacb1-066f-491a-b3e3-9423e93fb7cd))
  (fp_line (start 0.35 -1.55) (end 0.35 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4200f364-db7c-4de4-a0bb-c8a2f84e9a59))
  (fp_line (start 0.35 -0.95) (end 0.65 -0.95)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 754ea898-058c-43fc-9d56-eccbc1c69f0c))
  (fp_line (start 0.65 -1.55) (end 0.35 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 03f642c5-c523-46f8-a2c8-7e7c3b521149))
  (fp_line (start 0.65 -0.95) (end 0.65 -1.55)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 585692c1-c92c-4225-adb0-cca78026b1e0))
  (fp_line (start 2 1) (end 2 -1.9)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e4485e95-e1cb-4ee7-b02d-3decad1412b6))
  (pad "1" smd roundrect (at -0.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b7b5a20f-0ad3-4316-9af9-191f1072a546))
  (pad "2" smd roundrect (at 0.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4beda79a-21ac-44b6-b83c-97acda163c84))
  (pad "MP" smd roundrect (at -1.8 -1.2) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333) (tstamp 9138b230-c564-48bf-bd80-b7933710a0cb))
  (pad "MP" smd roundrect (at 1.8 -1.2) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333) (tstamp 48646e08-954f-4abe-aad6-91feb4506b99))
  (model ":KICAD7_3DMODEL_DIR:Connector_JST.3dshapes/JST_SH_BM02B-SRSS-TB.STEP"
    (offset (xyz 0 0.45 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
