(module CONN_JST_SUR_SM14B-SURS-TF (layer F.Cu) (tedit 5440EEB6)
  (attr smd)
  (fp_text reference CONN_JST_SUR_SM14B-SURS-TF (at -5.6 1.9) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_text value VAL** (at 2.7 1.9) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_line (start -6.7 -2.2) (end 6.7 -2.2) (layer Dwgs.User) (width 0.05))
  (fp_text user "board edge" (at 0 -1.9) (layer Cmts.User)
    (effects (font (size 0.6 0.6) (thickness 0.127)))
  )
  (fp_line (start -6.7 -1.35) (end 6.7 -1.35) (layer F.SilkS) (width 0.127))
  (fp_line (start 6.7 -1.35) (end 6.7 1.35) (layer F.SilkS) (width 0.127))
  (fp_line (start 6.7 1.35) (end -6.7 1.35) (layer F.SilkS) (width 0.127))
  (fp_line (start -6.7 1.35) (end -6.7 -1.35) (layer F.SilkS) (width 0.127))
)
