(footprint "JST_SH_SM15B-SRSS-TB_1x15-1MP_P1.00mm_Horizontal"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(locked yes)
	(layer "F.Cu")
	(descr "JST SH series connector, SM15B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
	(tags "connector JST SH horizontal")
	(property "Reference" "J6"
		(at 0 -3.98 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "ebc0ffcc-0dcf-4f20-9648-330097d2ff49")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "SERVO 1,2 / H-bridge"
		(at 0 3.98 0)
		(layer "F.Fab")
		(uuid "ce6077cd-8eb9-465b-8d57-d8b816f53de6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Connector_JST:JST_SH_SM15B-SRSS-TB_1x15-1MP_P1.00mm_Horizontal"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "063be8b9-d55c-4019-91ec-4588ecac8d86")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "aae74e7b-0cd4-406a-91dd-f2efef1e5dca")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Generic connectable mounting pin connector, single row, 01x15, script generated (kicad-library-utils/schlib/autogen/connector/)"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9ac0d340-e3f3-4829-988d-1d3ed143a5bf")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "JST"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "394bd298-7b6f-4f26-b429-6c1d7b4e41e2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "SM10B-SRSS-TB(LF)(SN)"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ac22c3e1-376e-4ed6-bf51-7023634eda50")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C160409"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "90ec34a7-e684-4f6f-aacc-1f907cbd4fd3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Dielectric" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "882b9caf-1623-40b9-aa55-9f1b6706f9f6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint_Density" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "894e7b96-610e-4b2c-aa9f-476edaa8b812")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint_Library" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a44a6b7b-b3f4-4bc0-abf9-930c222bc105")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "JLCPCB Part" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "601be1f7-8aaf-482c-ab66-1cdaec8ff736")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Mouser" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "500ebced-2623-4680-a6f9-bbbe170d626f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -7.65 2.6)
		(end 7.65 2.75)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "66071d2b-4c1a-4efc-9357-95e34e76863e")
	)
	(fp_arc
		(start -8.625 -1.725)
		(mid -8.603033 -1.778033)
		(end -8.55 -1.8)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "25ba2c6f-ce52-435f-a53a-b15a0633aee2")
	)
	(fp_arc
		(start -7.425 -1.875)
		(mid -7.446967 -1.821967)
		(end -7.5 -1.8)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "1badbea1-5d7b-4c6a-a4de-8308b3d06d4f")
	)
	(fp_arc
		(start 8.55 -1.8)
		(mid 8.603033 -1.778033)
		(end 8.625 -1.725)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "231ca224-c3a6-44ea-afb8-2b8abba3cab3")
	)
	(fp_poly
		(pts
			(xy 8.55 0.9) (xy 8.55 -1.725) (xy 7.5 -1.725) (xy 7.5 -1.875) (xy 8.55 -1.875) (xy 8.7 -1.725) (xy 8.7 0.9)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "d1d5c248-e47d-4510-82fa-9bdfba25bc0b")
	)
	(fp_poly
		(pts
			(xy -8.55 0.9) (xy -8.55 -1.725) (xy -7.5 -1.725) (xy -7.35 -1.875) (xy -7.35 -2.575) (xy -7.5 -2.575)
			(xy -7.5 -1.875) (xy -8.55 -1.875) (xy -8.7 -1.725) (xy -8.7 0.9)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "00d8d123-caa7-4984-8a90-51bf2365675c")
	)
	(fp_line
		(start -9 2.575)
		(end -9 1.175)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "88205967-b5cd-4c71-b818-b2ea4a0cc18d")
	)
	(fp_line
		(start -8.75 -1.675)
		(end -8.75 0.875)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "d27d98c9-d5e3-4537-8593-959d13dc0c60")
	)
	(fp_line
		(start -8.74932 0.879082)
		(end -8.75 0.875)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "0fe32d1b-925a-45e7-96d2-ddd4fb25e186")
	)
	(fp_line
		(start -7.4 -2.625)
		(end -7.4 -1.925)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "8d62240a-508f-416e-84eb-d179d7fec488")
	)
	(fp_line
		(start -7.4 -1.925)
		(end -8.5 -1.925)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "d4de198d-d55c-49bd-93f3-c1c3f6634921")
	)
	(fp_line
		(start -7.15 -2.875)
		(end 7.15 -2.875)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "cb2af5c6-b1bd-4758-ad40-1464ddfc0dea")
	)
	(fp_line
		(start 7.4 -2.625)
		(end 7.4 -1.925)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "32f98814-a64d-41e7-bc22-91901a902c00")
	)
	(fp_line
		(start 7.4 -1.925)
		(end 8.5 -1.925)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "808713d7-e283-4cc3-87a0-d6cb7bf96779")
	)
	(fp_line
		(start 8.7 2.875)
		(end -8.7 2.875)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f1d66327-f5b8-41f1-863f-4f958ea1f9e1")
	)
	(fp_line
		(start 8.74932 0.879082)
		(end 8.75 0.875)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "6308f545-705f-42a6-acac-2fb64bcf21f3")
	)
	(fp_line
		(start 8.75 -1.675)
		(end 8.75 0.875)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "2b9fe1e9-e73a-46ac-bef8-a964cd48a47c")
	)
	(fp_line
		(start 9 2.575)
		(end 9 1.175)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "4467775b-8040-4cfb-834f-0501461e56e7")
	)
	(fp_arc
		(start -9 1.175)
		(mid -8.928906 0.981088)
		(end -8.74932 0.879082)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "fdb88942-2935-46ee-8972-7fcc4cc8927f")
	)
	(fp_arc
		(start -8.75 -1.675)
		(mid -8.676777 -1.851777)
		(end -8.5 -1.925)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "066cb286-471f-486b-aa11-3ebe0cc1e573")
	)
	(fp_arc
		(start -8.7 2.875)
		(mid -8.912132 2.787132)
		(end -9 2.575)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "7caf95f2-ccb2-4f1c-b7b4-690079845344")
	)
	(fp_arc
		(start -7.4 -2.625)
		(mid -7.326777 -2.801777)
		(end -7.15 -2.875)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f6bf34a2-b215-476c-9cc1-a1c89ea7a2de")
	)
	(fp_arc
		(start 7.15 -2.875)
		(mid 7.326777 -2.801777)
		(end 7.4 -2.625)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "b1b835bc-d29d-4efd-aa9b-8bc6f85937de")
	)
	(fp_arc
		(start 8.5 -1.925)
		(mid 8.676777 -1.851777)
		(end 8.75 -1.675)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e6abef60-ff09-46c2-a6a7-392515e2b798")
	)
	(fp_arc
		(start 8.74932 0.879082)
		(mid 8.928906 0.981088)
		(end 9 1.175)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "dd9511a7-3132-4921-88c1-2ff104d4049c")
	)
	(fp_arc
		(start 9 2.575)
		(mid 8.912132 2.787132)
		(end 8.7 2.875)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "320638aa-ea15-4464-a447-aec32a1c873c")
	)
	(fp_line
		(start -8.5 -1.675)
		(end -8.5 2.575)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d67454f5-75bc-4517-82bf-abecae4d3af2")
	)
	(fp_line
		(start -8.5 -1.675)
		(end 8.5 -1.675)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "257705d9-2e37-409f-a246-6223a5fe1825")
	)
	(fp_line
		(start -8.5 2.575)
		(end 8.5 2.575)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0d080c72-410f-4410-a8ba-35601494ea1b")
	)
	(fp_line
		(start -7.5 -1.675)
		(end -7 -0.967893)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ce32ac9a-f5fd-44dd-b72b-7d67121788eb")
	)
	(fp_line
		(start -7 -0.967893)
		(end -6.5 -1.675)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "995f8507-f3e5-4d4e-bddf-8bf4a5929577")
	)
	(fp_line
		(start 8.5 -1.675)
		(end 8.5 2.575)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b7ddd734-248c-451d-b5f7-923e4876aa32")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "23b063fd-bb84-4b95-ac6f-f0b80a56785d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -7 -1.975)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(uuid "7b2af7c4-8ecb-40d8-9c29-eb2d51145f2e")
	)
	(pad "2" smd roundrect
		(at -6 -1.975)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(uuid "a3977862-d70d-494f-85ed-04167d0d3244")
	)
	(pad "3" smd roundrect
		(at -5 -1.975)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(uuid "856baf8b-957b-4b95-b03b-78e301dc3c71")
	)
	(pad "4" smd roundrect
		(at -4 -1.975)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(uuid "af84327c-f0b8-4d33-a7d8-66046966f29b")
	)
	(pad "5" smd roundrect
		(at -3 -1.975)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(uuid "ab1f0935-92aa-4a89-a13d-538c170ad74b")
	)
	(pad "6" smd roundrect
		(at -2 -1.975)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(uuid "e12291cd-a16b-4f9f-a4c9-5de2b742268d")
	)
	(pad "7" smd roundrect
		(at -1 -1.975)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(uuid "1eae3d44-ee07-4a42-af24-7a2f8d511b05")
	)
	(pad "8" smd roundrect
		(at 0 -1.975)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(uuid "99691b92-3f29-4261-bd82-fc4cf16ccaf8")
	)
	(pad "9" smd roundrect
		(at 1 -1.975)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(uuid "6df44086-c95d-467f-a63b-23c08a6075de")
	)
	(pad "10" smd roundrect
		(at 2 -1.975)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(uuid "a09f791b-aecc-4ddc-bb1f-1cd2bab4eb83")
	)
	(pad "11" smd roundrect
		(at 3 -1.975)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(uuid "fcddae54-7f21-4ec4-b598-7b33af2be887")
	)
	(pad "12" smd roundrect
		(at 4 -1.975)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(uuid "139599e0-b6d4-4c2e-a96a-c9369fe76e56")
	)
	(pad "13" smd roundrect
		(at 5 -1.975)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(uuid "27f05102-5c7a-4b90-9ed6-5ac8817ef3f5")
	)
	(pad "14" smd roundrect
		(at 6 -1.975)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(uuid "41121a3c-6b48-4c5f-8464-7475f8d7fb66")
	)
	(pad "15" smd roundrect
		(at 7 -1.975)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(uuid "2b3c750f-4cb9-44a5-88e2-85e478892ce6")
	)
	(pad "MP" smd roundrect
		(at -8.3 1.875)
		(size 1.1 1.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1363636364)
		(uuid "45c0209a-7d44-4322-afe1-37e371b976f9")
	)
	(pad "MP" smd roundrect
		(at 8.3 1.875)
		(size 1.1 1.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.1363636364)
		(uuid "61de4a03-a0e3-4d06-8df9-8a37ab80be63")
	)
	(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM15B-SRSS-TB_1x15-1MP_P1.00mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM15B-SRSS-TB.STEP"
		(offset
			(xyz 0 -0.45 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
