(footprint "TI_TMUX646_UCBGA-36_2.5x2.5mm_Layout6x6_P0.4mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "UCBGA-36, 6x6 raster, 2.5x2.5mm package, pitch 0.4mm; https://www.latticesemi.com/view_document?document_id=213")
	(tags "BGA 36 0.4")
	(property "Reference" "U4"
		(at 0 -2 180)
		(layer "F.SilkS")
		(hide yes)
		(uuid "79ddcba7-47ce-4e6e-b2ba-0c7f6bb227af")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "TI_TMUX646"
		(at 0.1 2.45 180)
		(layer "F.Fab")
		(uuid "1a7df5da-41c7-4644-8a14-77fe09a490be")
		(effects
			(font
				(size 0.2 0.2)
				(thickness 0.025)
			)
		)
	)
	(property "Footprint" "Package_BGA:TI_TMUX646_UCBGA-36_2.5x2.5mm_Layout6x6_P0.4mm"
		(at 0 0 0)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
		(uuid "7aa6e19b-25c8-4ddc-a2e4-a080f01a9da9")
		(effects
			(font
				(size 0.2 0.2)
				(thickness 0.025)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
		(uuid "973a809b-d119-4771-af6f-b2b70dd5e10a")
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify mirror)
		)
	)
	(property "Description" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
		(uuid "43c31ef0-d6d3-4a1e-b24a-012c8168e5be")
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify mirror)
		)
	)
	(property "LCSC" "C3656650"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "a168a8fa-ce13-4644-8908-7484bb07637c")
		(effects
			(font
				(size 0.2 0.2)
				(thickness 0.025)
			)
		)
	)
	(property "MFG" "TI"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "42e1f6c0-064d-41c2-acad-d649e8a41879")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "TMUX646ZECR"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "101e7f8b-7861-4e09-9df7-85f7366f80bc")
		(effects
			(font
				(size 0.2 0.2)
				(thickness 0.025)
			)
		)
	)
	(solder_mask_margin 0.035)
	(solder_paste_margin 0.000001)
	(clearance 0.09)
	(attr smd)
	(fp_line
		(start -1.36 -0.735)
		(end -1.36 1.36)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "09f20f52-9105-4fcb-9e10-1897e2d4be46")
	)
	(fp_line
		(start -1.36 1.36)
		(end 1.36 1.36)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2a3d3959-a33d-4987-b0db-a25059ceea78")
	)
	(fp_line
		(start 1.36 -1.36)
		(end -0.735 -1.36)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0e506d0e-2089-479d-87f4-0655851e2912")
	)
	(fp_line
		(start 1.36 1.36)
		(end 1.36 -1.36)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "847d8535-5121-48d7-bcc0-14d6abdfc974")
	)
	(fp_line
		(start -1.2 -0.8)
		(end -0.4 -0.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "3fc3e50c-388c-4ecb-92c2-a0ba9113ff73")
	)
	(fp_line
		(start -0.4 -1.2)
		(end -0.4 -0.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "3b1371bb-e3ee-4b21-936e-2a23fdb45b72")
	)
	(fp_line
		(start -0.4 -0.8)
		(end -0.4 1.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "944d1d62-dba9-4ceb-9e7c-4a8eb5c5b123")
	)
	(fp_line
		(start 0.4 -1.2)
		(end 0.4 -0.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "511e9237-d22d-438c-8799-de0dd7003d42")
	)
	(fp_line
		(start 0.4 -0.8)
		(end 1.2 -0.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "c3eb3acb-ade5-4f5a-9c85-304111adca7d")
	)
	(fp_line
		(start 0.4 -0.4)
		(end -0.4 0)
		(stroke
			(width 0.05)
			(type dash)
		)
		(layer "Dwgs.User")
		(uuid "af3d039b-30fe-4b4f-97d7-ba56e3d7e455")
	)
	(fp_line
		(start 0.4 0)
		(end -0.4 -0.4)
		(stroke
			(width 0.05)
			(type dash)
		)
		(layer "Dwgs.User")
		(uuid "8c8d6624-4e58-4b4a-b3a1-df1a3a45e6da")
	)
	(fp_line
		(start 0.4 1.2)
		(end 0.4 -0.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "87d727a1-5b82-4b74-a6c8-ca98b4dcf2fd")
	)
	(fp_line
		(start -0.6 0.4)
		(end -1 0.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "524686be-e576-47d3-be72-3b5fa61f4f77")
	)
	(fp_line
		(start -0.6 0.8)
		(end -1 0.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "b4a2f001-3448-4aaf-9781-a8e5a53e4635")
	)
	(fp_line
		(start -0.6 1.2)
		(end -1 1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "08541e74-d0dd-4365-a1f6-8d8945d30b3f")
	)
	(fp_line
		(start -0.2 -1)
		(end -1 -0.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "bf875e87-0cc4-4199-a2bd-72b4e5044883")
	)
	(fp_line
		(start -0.2 -0.6)
		(end -1 -0.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "ac622391-af35-4ca7-aa2c-2844b4ebaf13")
	)
	(fp_line
		(start -0.2 0)
		(end -0.6 0.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "f73f45b5-3f0a-4796-b79e-1bcb66da6752")
	)
	(fp_line
		(start -0.2 0.2)
		(end -0.6 0.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "cb716781-a03b-4383-bbad-df21d3119bba")
	)
	(fp_line
		(start -0.2 0.4)
		(end -0.6 0.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "2f7adbfb-73b5-4ff0-8c91-8e832838cfec")
	)
	(fp_line
		(start -0.2 0.6)
		(end -0.6 0.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "e1aff0a4-77a3-473c-a130-deedbdf8fc1c")
	)
	(fp_line
		(start -0.2 0.8)
		(end -0.6 1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "9ee3d7bf-9672-4907-bc62-f42eba1d3724")
	)
	(fp_line
		(start -0.2 1)
		(end -0.6 1.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "df169725-b080-453b-a0f2-195485e153c5")
	)
	(fp_line
		(start 0.2 -1)
		(end -0.6 -0.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "b1d0142c-1808-415f-9dc7-b5d3b0c64333")
	)
	(fp_line
		(start 0.2 -0.6)
		(end -0.6 -0.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "3b6618cc-5ded-4476-b862-540c9d70f80f")
	)
	(fp_line
		(start 0.2 0.2)
		(end -0.2 0)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "953785b0-4ffe-444f-929e-1423c1dc2b14")
	)
	(fp_line
		(start 0.2 0.4)
		(end -0.2 0.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "37d6bc09-db91-44ec-acb8-34c5e25691b7")
	)
	(fp_line
		(start 0.2 0.6)
		(end -0.2 0.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "1c3def2c-44f9-4a38-8a41-6f71e170d3f2")
	)
	(fp_line
		(start 0.2 0.8)
		(end -0.2 0.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "194c9837-d359-479f-98e4-6cc442cc9180")
	)
	(fp_line
		(start 0.2 1)
		(end -0.2 0.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "a9f39d3b-fe2b-482c-9455-d2ece255ef12")
	)
	(fp_line
		(start 0.2 1.2)
		(end -0.2 1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "86ae8c36-01a2-4906-bfff-4ab1880e4ef5")
	)
	(fp_line
		(start 0.6 -0.6)
		(end -0.2 -1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "01e38bd8-3fae-45a3-90c9-6ca464241669")
	)
	(fp_line
		(start 0.6 -0.2)
		(end -0.2 -0.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "3b5ad6c1-ac2c-465a-8677-bb2f0b585a82")
	)
	(fp_line
		(start 0.6 0)
		(end 0.2 0.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "4f4c5ae3-ecc2-48b4-bb1d-7c0d5a15bc1e")
	)
	(fp_line
		(start 0.6 0.2)
		(end 0.2 0.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "354bd0ef-fbba-477f-a8d4-5f0b11aac485")
	)
	(fp_line
		(start 0.6 0.4)
		(end 0.2 0.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "da4b6c0b-b942-48ce-b41b-ad946364ff2a")
	)
	(fp_line
		(start 0.6 0.6)
		(end 0.2 0.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "71a00dfa-9c55-4e82-89b7-b1ccb14f65c9")
	)
	(fp_line
		(start 0.6 0.8)
		(end 0.2 1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "a9ff2e80-d8dc-4805-8ae8-4df957f38fff")
	)
	(fp_line
		(start 0.6 1)
		(end 0.2 1.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "2434eea5-965b-4fe0-92fd-40d6ce5b0465")
	)
	(fp_line
		(start 1 -0.6)
		(end 0.2 -1)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "322ef939-54ef-4d10-9df1-31b3878316fa")
	)
	(fp_line
		(start 1 -0.2)
		(end 0.2 -0.6)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "2afddbef-becf-471f-93c6-c24446a771ac")
	)
	(fp_line
		(start 1 0.2)
		(end 0.6 0)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "6cde0374-5b5f-4ceb-8d8a-c89a4cd48059")
	)
	(fp_line
		(start 1 0.6)
		(end 0.6 0.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "4e81cbb6-4fe3-4484-afdb-a7174c0ed12d")
	)
	(fp_line
		(start 1 1)
		(end 0.6 0.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Cmts.User")
		(uuid "589db866-0b88-45f7-bedb-aca45ad8284f")
	)
	(fp_line
		(start -1.5 1.25)
		(end -1.5 -1.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "196a4a69-ce5e-4748-80c7-8a81fc790329")
	)
	(fp_line
		(start -1.25 -1.5)
		(end 1.25 -1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "1e8b7164-0e60-43d6-a78b-3b97bf161dcd")
	)
	(fp_line
		(start 1.25 1.5)
		(end -1.25 1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "cba11934-df63-4361-8532-c2aa036f6bba")
	)
	(fp_line
		(start 1.5 -1.25)
		(end 1.5 1.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "d0af1d15-800d-4c86-8828-8d1bb91ee7da")
	)
	(fp_arc
		(start -1.5 -1.25)
		(mid -1.426777 -1.426777)
		(end -1.25 -1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "b638bb63-e3cf-4cb5-ab98-613ca6379b39")
	)
	(fp_arc
		(start -1.25 1.5)
		(mid -1.426777 1.426777)
		(end -1.5 1.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f7c2e09f-4f30-4d9d-9d2c-fd3d2fa22693")
	)
	(fp_arc
		(start 1.25 -1.5)
		(mid 1.426777 -1.426777)
		(end 1.5 -1.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "432cf40f-8a8b-4716-b075-af65a2183425")
	)
	(fp_arc
		(start 1.5 1.25)
		(mid 1.426777 1.426777)
		(end 1.25 1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "a8c919dd-d1e9-4709-a99d-c4df6e56fc84")
	)
	(fp_line
		(start -1.25 -1.25)
		(end -1.25 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "00a55080-b3aa-44e9-9809-61edf196d45e")
	)
	(fp_line
		(start -1.25 1.25)
		(end 1.25 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4fc12dda-edac-4c1c-a485-f15e5989ca92")
	)
	(fp_line
		(start -0.625 -1.25)
		(end -1.25 -0.625)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "53e39854-0c96-4f80-b9d5-4f1829809b00")
	)
	(fp_line
		(start 1.25 -1.25)
		(end -1.25 -1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8e3964bf-3298-4bda-914f-d23eae14c2cb")
	)
	(fp_line
		(start 1.25 1.25)
		(end 1.25 -1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3fc72542-1951-4d52-8f89-1a27321fb7cf")
	)
	(fp_text user "OUTPUT A"
		(at 0.2 0 90)
		(unlocked yes)
		(layer "Dwgs.User")
		(uuid "139599cf-f9f8-4792-94b4-5db0eb8a97d5")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.05)
				(bold yes)
			)
			(justify bottom mirror)
		)
	)
	(fp_text user "OUTPUT B"
		(at -0.6 0.2 90)
		(unlocked yes)
		(layer "Dwgs.User")
		(uuid "2bccb282-5719-4a87-acc1-37dbbdde462d")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.05)
				(bold yes)
			)
			(justify bottom mirror)
		)
	)
	(fp_text user "INPUT"
		(at 1 0.2 90)
		(unlocked yes)
		(layer "Dwgs.User")
		(uuid "44983782-62c3-4701-aafe-1758dc0f8ea6")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.05)
				(bold yes)
			)
			(justify bottom mirror)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 -1.8 180)
		(layer "F.Fab")
		(uuid "b5d89231-96b7-45eb-9c3f-86caf17a2223")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.05)
				(bold yes)
			)
		)
	)
	(pad "A1" smd circle
		(at -1 -1)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "7db3d535-e3bc-4979-aec9-63847bb8f918")
	)
	(pad "A2" smd circle
		(at -0.6 -1)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "61489465-0ad6-476d-a722-ca3cdd3d1e14")
	)
	(pad "A3" smd circle
		(at -0.2 -1)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "ba747e31-3880-4f85-bcfc-cc9af7499457")
	)
	(pad "A4" smd circle
		(at 0.2 -1)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "4b6649ec-61a2-466a-b2d6-5f2ff7f75cde")
	)
	(pad "A5" smd circle
		(at 0.6 -1)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "80f8969b-f319-4628-8667-8a88a9099e8d")
	)
	(pad "A6" smd circle
		(at 1 -1)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "508ea794-7d26-429a-9778-62fc254a0849")
	)
	(pad "B1" smd circle
		(at -1 -0.6)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "1ab1583f-2f60-481d-893b-94566ae353f7")
	)
	(pad "B2" thru_hole circle
		(at -0.654 -0.654)
		(size 0.25 0.25)
		(drill 0.15)
		(layers "*.Cu")
		(remove_unused_layers yes)
		(keep_end_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "92332534-8924-4cfb-aabe-4732fbed9ef3")
	)
	(pad "B2" smd circle
		(at -0.6 -0.6)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "a88484f5-c286-47a4-a230-085d11adbf02")
	)
	(pad "B3" thru_hole circle
		(at -0.218 -0.65)
		(size 0.25 0.25)
		(drill 0.15)
		(layers "*.Cu")
		(remove_unused_layers yes)
		(keep_end_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "be33a185-cb5c-4ee0-ab13-e92e4f622263")
	)
	(pad "B3" smd circle
		(at -0.2 -0.6)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "b2eb10c5-7605-4873-aa73-5aaa596298bc")
	)
	(pad "B4" smd circle
		(at 0.2 -0.6)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "cfc4f7f8-94d9-4df0-823d-4fab73d21b0e")
	)
	(pad "B4" thru_hole circle
		(at 0.218 -0.65)
		(size 0.25 0.25)
		(drill 0.15)
		(layers "*.Cu")
		(remove_unused_layers yes)
		(keep_end_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "033a558f-044a-45d7-97ed-9062028ce499")
	)
	(pad "B5" smd circle
		(at 0.6 -0.6)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "ba0c23c9-dc3d-4cb2-a920-30b6b2b6f3a9")
	)
	(pad "B5" thru_hole circle
		(at 0.654 -0.654)
		(size 0.25 0.25)
		(drill 0.15)
		(layers "*.Cu")
		(remove_unused_layers yes)
		(keep_end_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "767c376f-f999-49d3-8d44-0d26869c8c00")
	)
	(pad "B6" smd circle
		(at 1 -0.6)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "e9dfaad1-9752-46c8-a548-3c4def1702b3")
	)
	(pad "C1" smd circle
		(at -1 -0.2)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "a2c4a2ba-cd2e-45df-baf4-bf36280de99b")
	)
	(pad "C2" thru_hole circle
		(at -0.65 -0.218)
		(size 0.25 0.25)
		(drill 0.15)
		(layers "*.Cu")
		(remove_unused_layers yes)
		(keep_end_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "178190ba-f343-409c-b399-7bf7ff441929")
	)
	(pad "C2" smd circle
		(at -0.6 -0.2)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "8863cbb6-9d05-4291-a6dd-55912b084663")
	)
	(pad "C3" smd circle
		(at -0.2 -0.2)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "3d4c69c2-57ba-4ca1-8d9f-fd20d62a9486")
	)
	(pad "C4" smd circle
		(at 0.2 -0.2)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "f705ee8e-9af7-4682-ace5-a257313b1542")
	)
	(pad "C5" smd circle
		(at 0.6 -0.2)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "0ab99a8f-10ca-4c37-9a0e-d342acd621c0")
	)
	(pad "C5" thru_hole circle
		(at 0.65 -0.218)
		(size 0.25 0.25)
		(drill 0.15)
		(layers "*.Cu")
		(remove_unused_layers yes)
		(keep_end_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "b490b20b-0d61-4e53-8475-edc226bc116a")
	)
	(pad "C6" smd circle
		(at 1 -0.2)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "e9629cca-4c0e-4c1b-85b3-988c7eb4ee2e")
	)
	(pad "D1" smd circle
		(at -1 0.2)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "861e1603-00a9-41ee-b9ae-a9694ea6880e")
	)
	(pad "D2" thru_hole circle
		(at -0.65 0.218)
		(size 0.25 0.25)
		(drill 0.15)
		(layers "*.Cu")
		(remove_unused_layers yes)
		(keep_end_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1bc0a677-79ed-44c6-b2b5-b5e3a05444e2")
	)
	(pad "D2" smd circle
		(at -0.6 0.2)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "cf0c18d3-9b49-4cb2-b492-689c7aa91dc1")
	)
	(pad "D3" thru_hole circle
		(at -0.2 0.2)
		(size 0.25 0.25)
		(drill 0.15)
		(layers "*.Cu")
		(remove_unused_layers yes)
		(keep_end_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "4a349d7a-8d5a-4065-9dc0-fdb9061e2094")
	)
	(pad "D3" smd circle
		(at -0.2 0.2)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "6348ae3a-82c3-4bcc-bb30-2dd0138dae44")
	)
	(pad "D4" thru_hole circle
		(at 0.2 0.2)
		(size 0.25 0.25)
		(drill 0.15)
		(layers "*.Cu")
		(remove_unused_layers yes)
		(keep_end_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "4e6800b8-202e-4174-8b9a-8ee36ee84843")
	)
	(pad "D4" smd circle
		(at 0.2 0.2)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "ce7886a1-b573-4dea-b4d8-c9177fa4ff2c")
	)
	(pad "D5" smd circle
		(at 0.6 0.2)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "654c4390-9b82-4e82-af1d-e37f9dc8b056")
	)
	(pad "D5" thru_hole circle
		(at 0.65 0.218)
		(size 0.25 0.25)
		(drill 0.15)
		(layers "*.Cu")
		(remove_unused_layers yes)
		(keep_end_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "72e105e2-5d55-4bbb-9018-aa8a483bd368")
	)
	(pad "D6" smd circle
		(at 1 0.2)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "f24e591c-945d-437a-99e2-430ac8e53816")
	)
	(pad "E1" smd circle
		(at -1 0.6)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "0983d2de-4947-42fd-b938-342873297d32")
	)
	(pad "E2" thru_hole circle
		(at -0.654 0.654)
		(size 0.25 0.25)
		(drill 0.15)
		(layers "*.Cu")
		(remove_unused_layers yes)
		(keep_end_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "ef456a8c-6b09-4e19-8420-a91d49adc5b8")
	)
	(pad "E2" smd circle
		(at -0.6 0.6)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "4248e39f-7586-479e-a411-1042264c016a")
	)
	(pad "E3" thru_hole circle
		(at -0.218 0.65)
		(size 0.25 0.25)
		(drill 0.15)
		(layers "*.Cu")
		(remove_unused_layers yes)
		(keep_end_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "14d90720-e79e-40cc-a15d-e85a8e704a98")
	)
	(pad "E3" smd circle
		(at -0.2 0.6)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "f766296d-3f92-418e-a822-13fe74b0257e")
	)
	(pad "E4" smd circle
		(at 0.2 0.6)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "81128977-861c-47ab-8ece-e2231bec7986")
	)
	(pad "E4" thru_hole circle
		(at 0.218 0.65)
		(size 0.25 0.25)
		(drill 0.15)
		(layers "*.Cu")
		(remove_unused_layers yes)
		(keep_end_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1e1aa3aa-2678-4a28-9e4a-330158e2da64")
	)
	(pad "E5" smd circle
		(at 0.6 0.6)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "d1456a26-9533-4e99-b30c-0e85a69d71c3")
	)
	(pad "E5" thru_hole circle
		(at 0.654 0.654)
		(size 0.25 0.25)
		(drill 0.15)
		(layers "*.Cu")
		(remove_unused_layers yes)
		(keep_end_layers no)
		(teardrops
			(best_length_ratio 0.5)
			(max_length 1)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "9ecd6a00-f330-481b-aa09-aacbccbb7b7b")
	)
	(pad "E6" smd circle
		(at 1 0.6)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "f1ffd3a4-d903-4917-b857-fd223abc856e")
	)
	(pad "F1" smd circle
		(at -1 1)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "51d43e4f-b222-4737-8471-196530527a2d")
	)
	(pad "F2" smd circle
		(at -0.6 1)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "aea93243-202e-4b79-a8dd-4c7719d1585c")
	)
	(pad "F3" smd circle
		(at -0.2 1)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "c47434ff-35d1-4ffe-9e08-6dacb686504a")
	)
	(pad "F4" smd circle
		(at 0.2 1)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "8151646b-95b7-4c06-be45-652a114bd438")
	)
	(pad "F5" smd circle
		(at 0.6 1)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "7600fbe8-a0e7-42e9-915a-8f0c437a9f46")
	)
	(pad "F6" smd circle
		(at 1 1)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "f6052ee5-c24b-48ab-9fb2-e49318efc0bc")
	)
	(model ":KICAD7_3DMODEL_DIR:Package_BGA.3dshapes/ucBGA-36_2.5x2.5mm_Layout6x6_P0.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)