(footprint "BarrierTerminalBlock_Cixi_KF88SA-16.0-2P"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "J18"
		(at 0 11.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "fa28befb-1cd2-4c19-8d05-e96b2613b250")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "48Vin"
		(at 0 -9.499999 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "53768ad2-21b3-4be6-8d63-7420e2a8f1bf")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "TerminalBlock:BarrierTerminalBlock_Cixi_KF88SA-16.0-2P"
		(at 0 -10.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3d95c0e4-882a-478c-ac83-868286b76f7d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 -10.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6af12504-a75f-4ab6-a76c-8164318f453f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
		(at 0 -10.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c24fa9fd-8c96-4caf-bc75-b8c7879b4fff")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C707749"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "35b2ec4d-ae25-4288-9eca-fa6bea78264c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "Cixi Kefa Elec"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c1eeb26a-18d8-4444-a96c-a91e2fbe7886")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "KF88SA-16.0-2P"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5629fbbd-4461-45a7-950d-847dc33b0f17")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Enable" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6767349f-c44d-4ac3-9cb9-2ff8da7ebacb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(zone_connect 2)
	(attr through_hole)
	(fp_poly
		(pts
			(xy -17.7 -10.5) (xy -17.7 10.5) (xy 17.7 10.5) (xy 17.7 -10.5)
		)
		(stroke
			(width 0.15)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "c7c17f8e-0c1e-4a61-b88f-ed85e086e377")
	)
	(fp_line
		(start -18.7 -10.5)
		(end -18.7 10.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "724d9a7d-268d-43f8-a224-1b8fd56e6f89")
	)
	(fp_line
		(start -17.7 11.5)
		(end 17.7 11.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "eacb5c00-cbdd-46fa-a562-b2d015a9448e")
	)
	(fp_line
		(start 17.7 -11.5)
		(end -17.7 -11.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "bf9e5f06-c7ff-4ecf-98ad-67460a476e76")
	)
	(fp_line
		(start 18.7 10.5)
		(end 18.7 -10.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e47ee629-a81a-4851-a694-e5d03c6c3b48")
	)
	(fp_arc
		(start -18.7 -10.5)
		(mid -18.407107 -11.207107)
		(end -17.7 -11.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "0717f7b1-8c86-428d-91c5-a9861020f271")
	)
	(fp_arc
		(start -17.7 11.5)
		(mid -18.407107 11.207107)
		(end -18.7 10.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "18fb1c19-ffe6-4856-9263-997b12344be8")
	)
	(fp_arc
		(start 17.7 -11.5)
		(mid 18.407107 -11.207107)
		(end 18.7 -10.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "2ca77214-3891-4310-ad07-ea6dd04d14a5")
	)
	(fp_arc
		(start 18.7 10.5)
		(mid 18.407107 11.207107)
		(end 17.7 11.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "23049cff-0462-431b-a35a-d227560b03f1")
	)
	(fp_poly
		(pts
			(xy -17.7 -10.5) (xy -17.7 10.5) (xy 17.7 10.5) (xy 17.7 -10.5)
		)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "2e8f7f68-754e-4506-a769-1013368ca167")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -8 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "aa2792d5-af73-460c-8565-83d505656fea")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole oval
		(at -8 -4.5)
		(size 6 2.3)
		(drill oval 5.5 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "034a27ce-0b65-46a9-a2e6-eec0a4044319")
	)
	(pad "1" connect oval
		(at -8 -4.5)
		(size 8.5 4.8)
		(layers "B.Cu" "B.Mask")
		(uuid "420828fe-8262-4f3a-a6fe-2c2bad18fb61")
	)
	(pad "1" thru_hole oval
		(at -8 4.5)
		(size 6 2.3)
		(drill oval 5.5 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "c7054b88-8ce4-42db-9872-55e8c1c7c977")
	)
	(pad "1" connect oval
		(at -8 4.5)
		(size 8.5 4.8)
		(layers "B.Cu" "B.Mask")
		(uuid "4699e674-0ab5-457d-8e3b-c0a8e309fef3")
	)
	(pad "2" thru_hole oval
		(at 8 -4.5)
		(size 6 2.3)
		(drill oval 5.5 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "62f37e52-8b4d-4172-91f4-874bbf6bf729")
	)
	(pad "2" connect oval
		(at 8 -4.5)
		(size 8.5 4.8)
		(layers "B.Cu" "B.Mask")
		(uuid "caa4b69a-ec26-4c3c-bc5a-2705bbbeadb2")
	)
	(pad "2" thru_hole oval
		(at 8 4.5)
		(size 6 2.3)
		(drill oval 5.5 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d81baf95-2410-434c-be4e-7ebb5aa778bd")
	)
	(pad "2" connect oval
		(at 8 4.5)
		(size 8.5 4.8)
		(layers "B.Cu" "B.Mask")
		(uuid "b1cca4db-b803-429a-a2a0-c8dc1af3fb0f")
	)
	(model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/CONN-TH_KF88SA-16.0-2P.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)