(footprint "QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "QFN, 48 Pin (http://www.st.com/resource/en/datasheet/stm32f042k6.pdf#page=94), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "QFN NoLead")
	(property "Reference" "B1F_U3"
		(at 0 -4.500001 180)
		(layer "F.SilkS")
		(hide yes)
		(uuid "3484553a-dc6d-49b2-8c89-56214f958d6d")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "STM32G431CBU6"
		(at 0 3.2 180)
		(layer "F.Fab")
		(uuid "80db58b7-8c7b-4e23-bb91-d9b69ace2c51")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.0625)
			)
		)
	)
	(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "80e4050a-80b5-437d-9d43-364029853052")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g473cb.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5b7e7428-ae06-4789-82d1-f157df50d3f3")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "91d37142-a69f-4c0f-a29d-f3872f0e0d7d")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C1342773"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "bb95888a-273c-48d5-9408-6da14385b581")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "ST"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "a28882ef-9ca8-44b4-aba7-e724f94a98c9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "STM32G473CEU6"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "208c79e4-9ab3-4e27-a2b4-e5d72a66194e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Preferred" ""
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "de254cf7-dc58-4d41-97d6-45c0b32df407")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "JLCPCB Rotation Offset" "180"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7df0fe2d-cc50-44cd-8621-e26bbd2d6833")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -3.61 3.61)
		(end -3.61 3.135)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4d14520d-8553-4336-a587-da8eef21c942")
	)
	(fp_line
		(start -3.135 -3.61)
		(end -3.61 -3.61)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "21c850d1-f309-46a9-93da-7cff2dfb4a5d")
	)
	(fp_line
		(start -3.135 3.61)
		(end -3.61 3.61)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a4275a4a-451a-4f1c-a424-3ecd4eb524e2")
	)
	(fp_line
		(start 3.135 -3.61)
		(end 3.61 -3.61)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5742338a-9688-4f5e-abb8-e7a03d766c50")
	)
	(fp_line
		(start 3.135 3.61)
		(end 3.61 3.61)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "04d3f368-590a-4144-8784-6bfb69f2d11b")
	)
	(fp_line
		(start 3.61 -3.61)
		(end 3.61 -3.135)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2b8ff0b0-405a-4807-9858-b9e36e6bcb53")
	)
	(fp_line
		(start 3.61 3.61)
		(end 3.61 3.135)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4fd327c7-0259-45df-a50a-ab910a1c3851")
	)
	(fp_line
		(start -4.05 -2.75)
		(end -4.05 2.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "d3a12380-0dce-4fdd-8ce3-8e4f21ce0486")
	)
	(fp_line
		(start -3.75 -3.5)
		(end -3.75 -3.05)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f3e7a3cd-ea12-4c1e-b7d3-918d5071c493")
	)
	(fp_line
		(start -3.75 3.5)
		(end -3.75 3.05)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "dd3ef543-69b6-4f4e-b8ff-3e822fa6c2ad")
	)
	(fp_line
		(start -3.5 -3.75)
		(end -3.05 -3.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "0cb0b67b-4add-4f5a-b387-cead20320693")
	)
	(fp_line
		(start -3.5 3.75)
		(end -3.05 3.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "fc5e3044-2b2f-4920-acd5-57ff1670ff9a")
	)
	(fp_line
		(start -2.75 4.05)
		(end 2.75 4.05)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "3b6b2b61-96be-4bd3-9304-469eefb9b8bd")
	)
	(fp_line
		(start 2.75 -4.05)
		(end -2.75 -4.05)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "91c584a3-2a8d-4051-a270-250e551f31a4")
	)
	(fp_line
		(start 3.5 -3.75)
		(end 3.05 -3.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5e6ff5e1-6e4c-4856-ab7d-ce258ff99c16")
	)
	(fp_line
		(start 3.5 3.75)
		(end 3.05 3.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5854a019-afa2-4583-923a-1c6ae1f3ec6c")
	)
	(fp_line
		(start 3.75 -3.5)
		(end 3.75 -3.05)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "7838bfd8-5bd0-4d0b-af05-792b566bdc25")
	)
	(fp_line
		(start 3.75 3.5)
		(end 3.75 3.05)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "71e2b233-d41c-426d-8f0e-adc3f6b90114")
	)
	(fp_line
		(start 4.05 2.75)
		(end 4.05 -2.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "39687632-64f4-47fd-9815-6498714465eb")
	)
	(fp_arc
		(start -4.05 -2.75)
		(mid -3.962132 -2.962132)
		(end -3.75 -3.05)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5c084a56-7671-4df8-be3f-1c961cba5047")
	)
	(fp_arc
		(start -3.75 -3.5)
		(mid -3.676777 -3.676777)
		(end -3.5 -3.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "0552cb92-edd8-422d-8aae-c6078746cd19")
	)
	(fp_arc
		(start -3.75 3.05)
		(mid -3.962132 2.962132)
		(end -4.05 2.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "99fb5367-99c0-4146-90cf-888459682d44")
	)
	(fp_arc
		(start -3.5 3.75)
		(mid -3.676777 3.676777)
		(end -3.75 3.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "bed233f8-9fc9-4416-b8f9-88de685cbda9")
	)
	(fp_arc
		(start -3.05 -3.75)
		(mid -2.962132 -3.962132)
		(end -2.75 -4.05)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "677fafe6-9d54-4bb3-aa9f-78669ee5beb7")
	)
	(fp_arc
		(start -2.75 4.05)
		(mid -2.962132 3.962132)
		(end -3.05 3.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "cca0e7f2-adc6-4a5b-b4ef-065760fa8d30")
	)
	(fp_arc
		(start 2.75 -4.05)
		(mid 2.962132 -3.962132)
		(end 3.05 -3.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "a7708e9f-fce8-4d10-8181-215fd7ec2422")
	)
	(fp_arc
		(start 3.05 3.75)
		(mid 2.962132 3.962132)
		(end 2.75 4.05)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "3bda6f02-0d4f-4879-8920-297afa8ae9f4")
	)
	(fp_arc
		(start 3.5 -3.75)
		(mid 3.676777 -3.676777)
		(end 3.75 -3.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "0d9f0864-f751-4f2f-a6ab-657765362d2d")
	)
	(fp_arc
		(start 3.75 -3.05)
		(mid 3.962132 -2.962132)
		(end 4.05 -2.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "3836dfcb-8a82-4570-8eda-93cd05587df0")
	)
	(fp_arc
		(start 3.75 3.5)
		(mid 3.676777 3.676777)
		(end 3.5 3.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "537756bc-d1e1-4380-a931-5a8ba54a33ff")
	)
	(fp_arc
		(start 4.05 2.75)
		(mid 3.962132 2.962132)
		(end 3.75 3.05)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "dc189551-f4ca-4bfb-ad82-98e8dc5e6ec4")
	)
	(fp_line
		(start -3.5 -2.5)
		(end -2.5 -3.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3d72a145-5d68-41ab-b433-1adb75b2e0f9")
	)
	(fp_line
		(start -3.5 3.5)
		(end -3.5 -2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8eb2f05a-4719-49ab-b725-0913d9617070")
	)
	(fp_line
		(start -2.5 -3.5)
		(end 3.5 -3.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b148de0b-f3a8-42eb-b877-444dfa250887")
	)
	(fp_line
		(start 3.5 -3.5)
		(end 3.5 3.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0d3eb631-39a0-46aa-ac04-a4ac26801a0f")
	)
	(fp_line
		(start 3.5 3.5)
		(end -3.5 3.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "429fd659-56f1-4bff-8c8d-818fd1051b7e")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -3.2 180)
		(layer "F.Fab")
		(uuid "43803e7d-9dbd-4429-bf74-cbc4b4e984a8")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.0625)
			)
		)
	)
	(pad "" smd oval
		(at -3.4375 -2.75)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "38d93a8c-6ba2-4387-8e8b-b65056f0c69c")
	)
	(pad "" smd oval
		(at -3.4375 -2.25)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "0557bc7d-71d7-4935-8bf0-b00665b66433")
	)
	(pad "" smd oval
		(at -3.4375 -1.749999)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "ff60ca0c-c0f3-4154-b231-c8495bc2ed52")
	)
	(pad "" smd oval
		(at -3.4375 -1.25)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1cff5b15-32b9-4d7b-a106-845c2e050c94")
	)
	(pad "" smd oval
		(at -3.4375 -0.750001)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "326af93f-9de0-4050-9f0a-fd2228c172c9")
	)
	(pad "" smd oval
		(at -3.4375 -0.25)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "0d0b5a29-e272-4db4-ba73-9b564ac5e7f9")
	)
	(pad "" smd oval
		(at -3.4375 0.25)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "f06bab99-42b3-40a1-9f69-fb05947f9ff9")
	)
	(pad "" smd oval
		(at -3.4375 0.750001)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "326d34a7-cab4-4536-8dbf-f8dd825c0e4f")
	)
	(pad "" smd oval
		(at -3.4375 1.25)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "13472ff6-897b-4627-a267-1fd8780c467e")
	)
	(pad "" smd oval
		(at -3.4375 1.749999)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "2685778e-7b97-4a16-8706-95645125f4c1")
	)
	(pad "" smd oval
		(at -3.4375 2.25)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "58c67060-704d-412f-a1d7-d7632f03b7e3")
	)
	(pad "" smd oval
		(at -3.4375 2.75)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "92d308e7-900c-4bde-8156-ada3baf1f4aa")
	)
	(pad "" smd oval
		(at -2.75 -3.4375 270)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "cc9a0c11-07bc-4797-b378-ca28b41c9a04")
	)
	(pad "" smd oval
		(at -2.75 3.4375 90)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "73c6659a-224f-4a95-8057-e37a11e555c9")
	)
	(pad "" smd oval
		(at -2.25 -3.4375 270)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "c25d7cb6-b702-45fd-ba7e-d12187325b85")
	)
	(pad "" smd oval
		(at -2.25 3.4375 90)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "a1492a0b-994d-4ced-b5ae-468eb9d91083")
	)
	(pad "" smd roundrect
		(at -2.1 -2.1)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.2212389381)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "bdbca038-5c81-40e3-89d0-451dba894a18")
	)
	(pad "" smd roundrect
		(at -2.1 -0.7)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.2212389381)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "06aeadac-f050-49b8-af7d-2da1a2f8f494")
	)
	(pad "" smd roundrect
		(at -2.1 0.7)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.2212389381)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "a9e68fb7-c021-45f4-88a8-abf4e4c42631")
	)
	(pad "" smd roundrect
		(at -2.1 2.1)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.2212389381)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "9b125dee-40fd-4054-82b3-64deb6ffbd50")
	)
	(pad "" smd oval
		(at -1.749999 -3.4375 270)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "0cb2f521-63c6-47a0-b30d-d22f3908a9b2")
	)
	(pad "" smd oval
		(at -1.749999 3.4375 90)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "92aa3e53-ef17-4038-8292-efecb6abb70a")
	)
	(pad "" smd oval
		(at -1.25 -3.4375 270)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "14b2719e-1e36-4a34-8535-8f92e656abff")
	)
	(pad "" smd oval
		(at -1.25 3.4375 90)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "e39d5c9a-e6fb-4a70-822b-ec273dc34eee")
	)
	(pad "" smd oval
		(at -0.750001 -3.4375 270)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "4ffd8041-4fd4-496e-ac59-12ea9c593fe4")
	)
	(pad "" smd oval
		(at -0.750001 3.4375 90)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "b6d1369e-03d0-4f81-9110-2e3fa5adaea0")
	)
	(pad "" smd roundrect
		(at -0.7 -2.1)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.2212389381)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "e49bd810-e6fc-4e9d-9f28-908a5f9ea5b5")
	)
	(pad "" smd roundrect
		(at -0.7 -0.7)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.2212389381)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "06d0655f-e378-4c55-b26f-f4122226a3c4")
	)
	(pad "" smd roundrect
		(at -0.7 0.7)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.2212389381)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "a2d213d4-654f-4798-b7f1-ae39f5f19a12")
	)
	(pad "" smd roundrect
		(at -0.7 2.1)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.2212389381)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "4fd6837a-7e7d-4c49-ab9f-0aba67f9906f")
	)
	(pad "" smd oval
		(at -0.25 -3.4375 270)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1231d6e2-6476-4dd6-9e2d-2e5cc525f7ad")
	)
	(pad "" smd oval
		(at -0.25 3.4375 90)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "cdaee9d2-f621-4371-8430-9f74a794bae7")
	)
	(pad "" smd oval
		(at 0.25 -3.4375 270)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "66d3fd56-4412-48de-af02-b541040bc311")
	)
	(pad "" smd oval
		(at 0.25 3.4375 90)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "3d5ef94f-48de-4a6c-ab4e-a13d77ff7ea0")
	)
	(pad "" smd roundrect
		(at 0.7 -2.1)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.2212389381)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "c44703b4-46ea-466a-b0c5-b23c2c677480")
	)
	(pad "" smd roundrect
		(at 0.7 -0.7)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.2212389381)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "3587dc6c-9f04-402d-9de2-4004da2c05cd")
	)
	(pad "" smd roundrect
		(at 0.7 0.7)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.2212389381)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "e9fe27ae-6e94-4f24-9508-aa874ae0b1aa")
	)
	(pad "" smd roundrect
		(at 0.7 2.1)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.2212389381)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "5926d80c-0d62-4dea-9b5b-0f7122049360")
	)
	(pad "" smd oval
		(at 0.750001 -3.4375 270)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "9ede5a60-821a-41ba-b972-f1c4d7c917f1")
	)
	(pad "" smd oval
		(at 0.750001 3.4375 90)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "f7e5f311-4c25-4d16-b2bf-c474b7e34e1b")
	)
	(pad "" smd oval
		(at 1.25 -3.4375 270)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1f43e78c-b124-482d-9676-4ebff496d845")
	)
	(pad "" smd oval
		(at 1.25 3.4375 90)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "9cd29871-b9e1-4eba-a6fc-d1a2440e62df")
	)
	(pad "" smd oval
		(at 1.749999 -3.4375 270)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "5ef2bf80-7a27-4c41-84e8-a8987588c922")
	)
	(pad "" smd oval
		(at 1.749999 3.4375 90)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "f11e0723-e518-464c-9c5c-7df0961effdc")
	)
	(pad "" smd roundrect
		(at 2.1 -2.1)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.2212389381)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "687d85a6-c0c6-49bb-b0a7-bdeda2256a71")
	)
	(pad "" smd roundrect
		(at 2.1 -0.7)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.2212389381)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "bfbc1f1d-c2f4-47d2-9bb8-e4616dd13d10")
	)
	(pad "" smd roundrect
		(at 2.1 0.7)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.2212389381)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "5f08f025-0583-4288-b488-26275e628e30")
	)
	(pad "" smd roundrect
		(at 2.1 2.1)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.2212389381)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "74814f09-4992-4cfb-b968-357bfae01027")
	)
	(pad "" smd oval
		(at 2.25 -3.4375 270)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "130962e1-0869-459d-b930-b2389a66dd5d")
	)
	(pad "" smd oval
		(at 2.25 3.4375 90)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "e3b189fe-eb69-4382-b499-1487796f704e")
	)
	(pad "" smd oval
		(at 2.75 -3.4375 270)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "b83eccdb-159f-4188-9278-ac72284386c8")
	)
	(pad "" smd oval
		(at 2.75 3.4375 90)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "8bd3dc93-1d01-4eec-9de4-0fad852f3fbf")
	)
	(pad "" smd oval
		(at 3.4375 -2.75 180)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "08d147ff-01b3-49d7-b8a0-29771de0babd")
	)
	(pad "" smd oval
		(at 3.4375 -2.25 180)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "16fc341e-c7db-450a-85f8-606c01952748")
	)
	(pad "" smd oval
		(at 3.4375 -1.749999 180)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "fd1bedf7-b2a3-439f-9eb6-3854cac00602")
	)
	(pad "" smd oval
		(at 3.4375 -1.25 180)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1c037a58-0841-4a12-9232-2323c11f6249")
	)
	(pad "" smd oval
		(at 3.4375 -0.750001 180)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "dadfbe41-9e71-4f4d-aa11-1b2d7fb219e6")
	)
	(pad "" smd oval
		(at 3.4375 -0.25 180)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "afb8f5b8-0363-4843-9805-42bfb54d56e3")
	)
	(pad "" smd oval
		(at 3.4375 0.25 180)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "9d9e0a7f-71ac-414b-beb9-044c30cfd25a")
	)
	(pad "" smd oval
		(at 3.4375 0.750001 180)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "712e061f-6455-4e0d-8b7c-17aaec5adcb1")
	)
	(pad "" smd oval
		(at 3.4375 1.25 180)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "d0043171-1841-4217-897e-4a3d8ef8f10b")
	)
	(pad "" smd oval
		(at 3.4375 1.749999 180)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "925c8318-91a4-4d0d-b98d-408e331d0564")
	)
	(pad "" smd oval
		(at 3.4375 2.25 180)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "ac9a605a-2517-47d7-acc2-d082ac1c2ee7")
	)
	(pad "" smd oval
		(at 3.4375 2.75 180)
		(size 0.7 0.2)
		(layers "F.Paste")
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "65395e9e-3866-4f04-b666-793f47ed6c66")
	)
	(pad "1" smd roundrect
		(at -3.4375 -2.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "a129360a-ee34-4e6b-b5ef-decd57fb8e61")
	)
	(pad "2" smd roundrect
		(at -3.4375 -2.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "6f9c68e8-5323-431c-9ca7-82bd4cf097c6")
	)
	(pad "3" smd roundrect
		(at -3.4375 -1.749999)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "d6280acd-63b8-48bb-aa77-caf76d548b60")
	)
	(pad "4" smd roundrect
		(at -3.4375 -1.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "b8582def-2284-40b2-9e0e-c780c9e464a7")
	)
	(pad "5" smd roundrect
		(at -3.4375 -0.750001)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "840175df-169a-4e3e-8deb-f17e3e3e4b2c")
	)
	(pad "6" smd roundrect
		(at -3.4375 -0.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "015c8bbf-2dc4-42cd-beb9-34c9e89eb445")
	)
	(pad "7" smd roundrect
		(at -3.4375 0.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "971e3dc8-b5b2-42b0-8680-97617aaf7575")
	)
	(pad "8" smd roundrect
		(at -3.4375 0.750001)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "7ae2084f-1db5-4e64-b8c1-d594fbd3cd59")
	)
	(pad "9" smd roundrect
		(at -3.4375 1.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "8b3833fa-5728-4746-8a6e-e894677d865c")
	)
	(pad "10" smd roundrect
		(at -3.4375 1.749999)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "9665a567-905b-4b8d-b5e9-55cd1710ce44")
	)
	(pad "11" smd roundrect
		(at -3.4375 2.25)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "ec1881cf-8626-4c13-aa32-aef46d12a7e0")
	)
	(pad "12" smd roundrect
		(at -3.4375 2.75)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "996997ce-940f-4463-a61c-b2f0a64324f1")
	)
	(pad "13" smd roundrect
		(at -2.75 3.4375 90)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "56b1f9be-326f-4eab-8f39-da83745b5d40")
	)
	(pad "14" smd roundrect
		(at -2.25 3.4375 90)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "e71bb153-c8e6-45fe-a543-ec45dcc952e9")
	)
	(pad "15" smd roundrect
		(at -1.749999 3.4375 90)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "aee8828e-46ed-4f81-8599-155055700bd4")
	)
	(pad "16" smd roundrect
		(at -1.25 3.4375 90)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "73c67f5d-d440-4476-9057-8885527c2aac")
	)
	(pad "17" smd roundrect
		(at -0.750001 3.4375 90)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "9c6ac3f0-5cac-4345-a805-d930e5fd425d")
	)
	(pad "18" smd roundrect
		(at -0.25 3.4375 90)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "961748e1-a8c5-48fc-b0cb-e726b3ef7907")
	)
	(pad "19" smd roundrect
		(at 0.25 3.4375 90)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "2b9621db-2183-4e46-b12e-0774e77c8c8d")
	)
	(pad "20" smd roundrect
		(at 0.750001 3.4375 90)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "e0a03e76-da2f-4046-acf0-c3145ab12773")
	)
	(pad "21" smd roundrect
		(at 1.25 3.4375 90)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1807af1c-b3e9-4c71-a4eb-edc1f9c13efa")
	)
	(pad "22" smd roundrect
		(at 1.749999 3.4375 90)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "efd165b5-2bfb-4768-ad65-0bb93dc14d61")
	)
	(pad "23" smd roundrect
		(at 2.25 3.4375 90)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "38fc24b0-ca13-4ea2-a17a-9d1120684f9d")
	)
	(pad "24" smd roundrect
		(at 2.75 3.4375 90)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "392ae341-f688-4a89-aaab-f5da74ca9736")
	)
	(pad "25" smd roundrect
		(at 3.4375 2.75 180)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "272a86fe-6290-4b5e-ba7b-ad5b1b39f594")
	)
	(pad "26" smd roundrect
		(at 3.4375 2.25 180)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "c7418e1d-ddd9-4e2b-8e69-e4cf45e5a82b")
	)
	(pad "27" smd roundrect
		(at 3.4375 1.749999 180)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "602e570f-c4bb-456c-9461-f6250b1daef7")
	)
	(pad "28" smd roundrect
		(at 3.4375 1.25 180)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "7c18416a-074c-4d17-853e-f90e5f19aa6f")
	)
	(pad "29" smd roundrect
		(at 3.4375 0.750001 180)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "f7c0ede2-1ab5-4d3f-83ed-a455afdda5aa")
	)
	(pad "30" smd roundrect
		(at 3.4375 0.25 180)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "82932961-fe2b-492c-8d5f-b942d7f3d1ac")
	)
	(pad "31" smd roundrect
		(at 3.4375 -0.25 180)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "c02b11a4-5f9f-4a72-89ad-65b5f82d6ad3")
	)
	(pad "32" smd roundrect
		(at 3.4375 -0.750001 180)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "157141d7-604c-4be7-9770-c78de019037f")
	)
	(pad "33" smd roundrect
		(at 3.4375 -1.25 180)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "f866674a-9f4c-420b-b8e3-5ba32e04e608")
	)
	(pad "34" smd roundrect
		(at 3.4375 -1.749999 180)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "dfc3d320-3666-4fc8-93e7-442893db3c47")
	)
	(pad "35" smd roundrect
		(at 3.4375 -2.25 180)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "332917a6-1376-4143-9587-9288dcafc584")
	)
	(pad "36" smd roundrect
		(at 3.4375 -2.75 180)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "a09e25ca-5769-4b58-8150-344cbe1913a0")
	)
	(pad "37" smd roundrect
		(at 2.75 -3.4375 270)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "2c46d254-13cb-4f5e-82e5-61a7d75868b8")
	)
	(pad "38" smd roundrect
		(at 2.25 -3.4375 270)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "42e1a0ff-b2c0-4585-8ed4-7eddd259afb7")
	)
	(pad "39" smd roundrect
		(at 1.749999 -3.4375 270)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "57748716-ca03-4e1b-9708-dc60827f038e")
	)
	(pad "40" smd roundrect
		(at 1.25 -3.4375 270)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1d576701-5b75-4e4d-b621-b959f34b40a0")
	)
	(pad "41" smd roundrect
		(at 0.750001 -3.4375 270)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "220b04a5-c3a1-4983-8dbf-76ccd8ccdbde")
	)
	(pad "42" smd roundrect
		(at 0.25 -3.4375 270)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "3ceb27d1-c8ed-4b4f-ba16-0a18be9c6c2f")
	)
	(pad "43" smd roundrect
		(at -0.25 -3.4375 270)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "11e8bed3-ca00-49f8-b914-d543b0c8a4f7")
	)
	(pad "44" smd roundrect
		(at -0.750001 -3.4375 270)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "b1236956-f7c2-433d-bfdf-34e30f9a68e5")
	)
	(pad "45" smd roundrect
		(at -1.25 -3.4375 270)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "d5cf9997-6824-4c25-a8b2-821a508b7cc5")
	)
	(pad "46" smd roundrect
		(at -1.749999 -3.4375 270)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "2dcfcf81-2838-4acf-993c-d506d03b8302")
	)
	(pad "47" smd roundrect
		(at -2.25 -3.4375 270)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "de56cf17-47a8-4704-a2f1-d4a9bcb06b36")
	)
	(pad "48" smd roundrect
		(at -2.75 -3.4375 270)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.1)
		(chamfer top_right bottom_right)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "da90cd48-ea42-428a-95b5-f8498da51222")
	)
	(pad "49" smd roundrect
		(at 0 0)
		(size 5.6 5.6)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.01785714286)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "34b737a9-cde2-423d-b7fe-193c4a617ba8")
	)
	(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm.wrl"
		(hide yes)
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
