(module Diode_Bridge_18.5x5.5 (layer F.Cu) (tedit 5943D578)
  (descr "Single phase bridge rectifier case 18.5x5.5")
  (tags "Diode Bridge")
  (fp_text reference D1 (at -9.9 -3.3) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Bridge_Rectifier (at -3.7 4.8) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at -0.175 2.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 6.95 2.5) (end 7.95 2.5) (layer F.Fab) (width 0.1))
  (fp_line (start -8.3 2.5) (end -7.3 2.5) (layer F.Fab) (width 0.1))
  (fp_line (start -7.8 2) (end -7.8 3) (layer F.Fab) (width 0.1))
  (fp_line (start 11.65 -2.6) (end 11.65 3.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start 11.65 3.9) (end -12.45 3.9) (layer F.CrtYd) (width 0.05))
  (fp_line (start -12.45 3.9) (end -12.45 -2.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -12.45 -2.6) (end 11.65 -2.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -12.1 -2.25) (end 11.3 -2.25) (layer F.SilkS) (width 0.15))
  (fp_line (start 11.3 -2.25) (end 11.3 3.55) (layer F.SilkS) (width 0.15))
  (fp_line (start 11.3 3.55) (end -12.1 3.55) (layer F.SilkS) (width 0.15))
  (fp_line (start -12.1 3.55) (end -12.1 -2.25) (layer F.SilkS) (width 0.15))
  (fp_arc (start 2.25 2.2) (end 2.55 2.5) (angle 100) (layer F.Fab) (width 0.1))
  (fp_arc (start 2.9 2.7) (end 2.55 2.5) (angle 100) (layer F.Fab) (width 0.1))
  (fp_arc (start -2.2 2.7) (end -2.55 2.5) (angle 100) (layer F.Fab) (width 0.1))
  (fp_arc (start -2.85 2.2) (end -2.55 2.5) (angle 100) (layer F.Fab) (width 0.1))
  (pad + thru_hole rect (at -7.8 0) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask))
  (pad A+ thru_hole circle (at -2.7 0) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask))
  (pad - thru_hole circle (at 7.5 0) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask))
  (pad A- thru_hole circle (at 2.4 0) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask))
  (model ${KICAD7_3DMODEL_DIR}/Diodes_THT.3dshapes/Diode_Bridge_18_5x5_5.wrl
    (at (xyz -0.3070866141732284 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
