(footprint "X2-DFN0806-6"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.97 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "ada76672-1039-4edf-a4a1-fa7bc80e6a4f")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.15)
				(bold yes)
			)
		)
	)
	(property "Value" "X2-DFN0806-6"
		(at 0 0.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "56efb967-8806-45fb-b2d7-93898bf1757d")
		(effects
			(font
				(size 0.1 0.1)
				(thickness 0.025)
				(bold yes)
			)
		)
	)
	(property "Footprint" ""
		(at 0 -2.34 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "410f7a12-4f4f-461d-b62b-7d61c1c1afd3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 -2.34 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0d5f7b81-05b8-4101-b5c5-512f8fc5149e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 -2.34 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5bcaf956-bed7-4e71-8891-235ff2756125")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -0.6 -0.3)
		(end -0.45 0.075)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "bdd9f8e6-770f-47ae-86f3-fec2b8c03eb3")
	)
	(fp_rect
		(start 0.45 -0.075)
		(end 0.6 0.3)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "c0a3ede5-9974-42a8-b4fa-ff1481d3f45f")
	)
	(fp_poly
		(pts
			(xy -0.35 0.475) (xy -0.45 0.6) (xy -0.25 0.6)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "547948ab-9622-48da-bed5-240559c143c1")
	)
	(fp_line
		(start -0.575 0.375)
		(end -0.575 -0.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "01a1fea6-bc61-4632-a0fa-634d8148fab5")
	)
	(fp_line
		(start -0.375 0.575)
		(end 0.35 0.575)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "13a59ed2-dc76-4d56-bca1-46dc4b920ced")
	)
	(fp_line
		(start 0.375 -0.575)
		(end -0.35 -0.575)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5cabf174-40ca-425a-b46e-017d545c336b")
	)
	(fp_line
		(start 0.575 -0.375)
		(end 0.575 0.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f8611275-eaf0-400b-befc-7f39d49caa03")
	)
	(fp_arc
		(start -0.575 -0.35)
		(mid -0.509099 -0.509099)
		(end -0.35 -0.575)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "87a4b7ab-2d00-415f-b67e-899aa8256d86")
	)
	(fp_arc
		(start -0.375 0.575)
		(mid -0.516421 0.516421)
		(end -0.575 0.375)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ee7b0ca3-a92f-41dd-b865-47d5a4a2cf1a")
	)
	(fp_arc
		(start 0.375 -0.575)
		(mid 0.516421 -0.516421)
		(end 0.575 -0.375)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e105e2a2-db53-4358-9449-39fef24b8d32")
	)
	(fp_arc
		(start 0.575 0.35)
		(mid 0.509099 0.509099)
		(end 0.35 0.575)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "7418b744-fad9-4b1b-b6ef-4f9601cc75cd")
	)
	(fp_rect
		(start -0.4 -0.3)
		(end 0.4 0.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "581ca1af-5613-4834-bd87-b4b558b5a217")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0.65 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "f9605e08-8d8a-49ee-80ae-851903dd94f1")
		(effects
			(font
				(size 0.1 0.1)
				(thickness 0.025)
				(bold yes)
			)
		)
	)
	(pad "" smd oval
		(at -0.35 0.262)
		(size 0.15 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "e5645f59-f817-468c-9812-87cf288383a1")
	)
	(pad "" smd oval
		(at -0.275 -0.227 180)
		(size 0.2 0.275)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "ef00b19f-2024-44e7-981c-ccc4c240a860")
	)
	(pad "" smd oval
		(at -0.05 0.27)
		(size 0.15 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "f40b4b01-2de1-4b11-8707-d75683f2593b")
	)
	(pad "" smd oval
		(at 0.05 -0.27 180)
		(size 0.15 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "f9b5c0d0-7b28-40c0-90ca-058e022a70a9")
	)
	(pad "" smd oval
		(at 0.275 0.227)
		(size 0.2 0.275)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "b804524b-882f-438b-a7a8-7061be70d52a")
	)
	(pad "" smd oval
		(at 0.35 -0.262 180)
		(size 0.15 0.225)
		(layers "F.Paste")
		(thermal_bridge_angle 45)
		(uuid "ddb30357-338a-4edd-b2c1-0a2dda950f8a")
	)
	(pad "1" smd roundrect
		(at -0.35 0.262)
		(size 0.15 0.275)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_left top_right)
		(thermal_bridge_angle 45)
		(uuid "d21bd048-e722-44ec-b092-a8a8faedb5b0")
	)
	(pad "2" smd roundrect
		(at -0.05 0.262)
		(size 0.15 0.275)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_left top_right)
		(thermal_bridge_angle 45)
		(uuid "1ecbd59c-0ed4-45f1-90d3-e9a2cec3b153")
	)
	(pad "3" smd roundrect
		(at 0.275 0.227)
		(size 0.2 0.345)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_left top_right)
		(thermal_bridge_angle 45)
		(uuid "981ba263-3a69-45c4-b610-edab519c6322")
	)
	(pad "4" smd roundrect
		(at 0.35 -0.262 180)
		(size 0.15 0.275)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_left top_right)
		(thermal_bridge_angle 45)
		(uuid "e1de7f02-d1c0-4334-ac1e-76807b9e563a")
	)
	(pad "5" smd roundrect
		(at 0.05 -0.262 180)
		(size 0.15 0.275)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_left top_right)
		(thermal_bridge_angle 45)
		(uuid "f4e609db-c1c7-4933-a0cc-d1a5f8c584a6")
	)
	(pad "6" smd roundrect
		(at -0.275 -0.227 180)
		(size 0.2 0.345)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.33)
		(chamfer_ratio 0.05)
		(chamfer top_left top_right)
		(thermal_bridge_angle 45)
		(uuid "11683efc-8b20-49e4-a764-6a35ae0150ce")
	)
	(model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN0806H4-6.stp"
		(opacity 0.6800)
		(offset
			(xyz 0 0 0.4)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
