(footprint "1265"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "L1"
		(at 0 -6.75 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "68a88361-3f0b-46a9-ae57-16c28139238e")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.125)
			)
		)
	)
	(property "Value" "5.6uH"
		(at 0 -5.5 180)
		(layer "F.Fab")
		(uuid "4aca5f11-da0c-4093-b9cc-489cc1c4067d")
		(effects
			(font
				(size 0.6 0.6)
				(thickness 0.125)
			)
		)
	)
	(property "Footprint" "1265"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "44a97a33-bae6-4688-b90e-13783a6871a5")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "529432b3-77fa-4db8-8d28-2ac41a2c419a")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "623681e6-f267-4cac-867e-79e3d3a1d51e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "TAI-TECH"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "3bbeb007-08fb-45c5-9d8c-3eca644f6b04")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "TMPC1265HP-5R6MG-D"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "8a0386a0-d01d-43c0-b547-a53e6ee2014c")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C357274"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "96445c31-d479-4a78-82b9-6eb1b9fed377")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "PCBA" "x"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "55b3ba2a-1862-4959-8b0f-561db64a0f23")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Preferred" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4faa42f5-5b1d-4ec5-9339-df69e9dff5f9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(zone_connect 2)
	(attr smd)
	(fp_arc
		(start -6.825 -6.3)
		(mid -6.803033 -6.353033)
		(end -6.75 -6.375)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "cc91692d-ad29-44a6-881e-be4ddef4bb74")
	)
	(fp_arc
		(start -6.75 6.375)
		(mid -6.803033 6.353033)
		(end -6.825 6.3)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "72048d6e-be52-4225-96fe-91fa8c34ee21")
	)
	(fp_arc
		(start 6.75 -6.375)
		(mid 6.803033 -6.353033)
		(end 6.825 -6.3)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "93ab1b9d-9027-48d1-9947-ca7bb08248eb")
	)
	(fp_arc
		(start 6.825 6.3)
		(mid 6.803033 6.353033)
		(end 6.75 6.375)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d873f01b-f584-4cde-9514-4c2c9c4cfba4")
	)
	(fp_poly
		(pts
			(xy -6.75 -6.3) (xy -5.1 -6.3) (xy -5.1 -6.45) (xy -6.75 -6.45) (xy -6.9 -6.3) (xy -6.9 -4.8) (xy -6.75 -4.8)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "5d3a5e53-d7d9-47ff-9669-dde133ec2b71")
	)
	(fp_poly
		(pts
			(xy -6.75 6.3) (xy -6.75 4.65) (xy -6.9 4.65) (xy -6.9 6.3) (xy -6.75 6.45) (xy -5.25 6.45) (xy -5.25 6.3)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "fc8f699e-1d4e-42dd-84f9-b13b98835115")
	)
	(fp_poly
		(pts
			(xy 6.75 -6.3) (xy 6.75 -4.65) (xy 6.9 -4.65) (xy 6.9 -6.3) (xy 6.75 -6.45) (xy 5.25 -6.45) (xy 5.25 -6.3)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "a72e2b05-6757-47fd-8f9f-e4b03ceb1dfd")
	)
	(fp_poly
		(pts
			(xy 6.75 6.3) (xy 5.1 6.3) (xy 5.1 6.45) (xy 6.75 6.45) (xy 6.9 6.3) (xy 6.9 4.8) (xy 6.75 4.8)
		)
		(stroke
			(width 0)
			(type solid)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "734c08a7-fa82-4720-971c-263d0ca70843")
	)
	(fp_line
		(start -7.3 2.45)
		(end -7.3 -2.45)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e13974f9-6421-4f62-bb9d-51b504c7de8a")
	)
	(fp_line
		(start -6.9 -6.4)
		(end -6.9 -2.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "345a3710-e058-4d1b-b5b6-b2ea179e89f3")
	)
	(fp_line
		(start -6.9 -2.75)
		(end -7 -2.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "6a653def-560a-4998-9a98-8d6a5a29e7a8")
	)
	(fp_line
		(start -6.9 2.75)
		(end -7 2.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "513ceb07-94fa-461e-b55b-0bea60ba4354")
	)
	(fp_line
		(start -6.9 6.4)
		(end -6.9 2.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "1400dbca-fa33-494f-a309-90012c4528b9")
	)
	(fp_line
		(start -6.75 -6.55)
		(end 6.75 -6.55)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9a11d3f7-edd2-4e06-90ad-a93a6f5f921a")
	)
	(fp_line
		(start -6.75 6.55)
		(end 6.75 6.55)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "a255c2de-8233-4205-90ea-8628f3e941d1")
	)
	(fp_line
		(start 6.9 -6.4)
		(end 6.9 -2.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e5435d28-619d-4503-83bc-dbd05a7be7ec")
	)
	(fp_line
		(start 6.9 -2.75)
		(end 7 -2.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9a0c8346-b1a6-4567-a09c-9bca87a2ee4c")
	)
	(fp_line
		(start 6.9 2.75)
		(end 7 2.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ec3067ba-2110-44c2-a004-4d06ef2890da")
	)
	(fp_line
		(start 6.9 6.4)
		(end 6.9 2.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "88a19150-5492-44ab-bd70-02686894a9c2")
	)
	(fp_line
		(start 7.3 -2.45)
		(end 7.3 2.45)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "4b46b55c-e4e5-4427-ba84-93f9c91a7dd6")
	)
	(fp_arc
		(start -7.3 -2.45)
		(mid -7.212132 -2.662132)
		(end -7 -2.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "3d5821b1-8c73-4727-beb4-32e3204f54f0")
	)
	(fp_arc
		(start -7 2.75)
		(mid -7.212132 2.662132)
		(end -7.3 2.45)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "60d38800-f3c2-4311-a804-1079d51a9262")
	)
	(fp_arc
		(start -6.9 -6.4)
		(mid -6.856066 -6.506066)
		(end -6.75 -6.55)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "6b808417-7a5f-4e03-9998-c7f7eb2fe643")
	)
	(fp_arc
		(start -6.75 6.55)
		(mid -6.856066 6.506066)
		(end -6.9 6.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "2205d887-c618-4366-8a06-e30c6cf598d5")
	)
	(fp_arc
		(start 6.75 -6.55)
		(mid 6.856066 -6.506066)
		(end 6.9 -6.4)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "a9ef87e9-297e-483e-82c5-164253ca4dbe")
	)
	(fp_arc
		(start 6.9 6.4)
		(mid 6.856066 6.506066)
		(end 6.75 6.55)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "99ff04da-ab6a-4fd6-9435-7f608423d9a8")
	)
	(fp_arc
		(start 7 -2.75)
		(mid 7.212132 -2.662132)
		(end 7.3 -2.45)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "70f93ade-b024-4770-b5f9-24ea912fee35")
	)
	(fp_arc
		(start 7.3 2.45)
		(mid 7.212132 2.662132)
		(end 7 2.75)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "56a62b6f-e045-43ca-a33e-015755211003")
	)
	(fp_line
		(start -7 -2.5)
		(end -6.75 -2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "b2bf75ab-eb00-4688-868d-bd2dbe3de5d6")
	)
	(fp_line
		(start -7 2.5)
		(end -7 -2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "a45063c1-7690-43f5-a47a-468d0b5f24e8")
	)
	(fp_line
		(start -6.75 -6.25)
		(end -6.75 -2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "f34b9dde-de8e-43ae-b51e-aacb1a6faa3b")
	)
	(fp_line
		(start -6.75 -2.5)
		(end -6.25 -2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "ccfa1ab7-62f1-4a40-996a-1e75b126fc59")
	)
	(fp_line
		(start -6.75 2.5)
		(end -7 2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "515ab54a-c822-4629-ae47-f13b347bacff")
	)
	(fp_line
		(start -6.75 2.5)
		(end -6.75 -2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "737a39f0-6fad-416a-8b4c-2bf87fcd9c7c")
	)
	(fp_line
		(start -6.75 6.25)
		(end -6.75 2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "55e65825-19bc-4721-ac24-419368b783f6")
	)
	(fp_line
		(start -6.25 -6.25)
		(end -6.75 -6.25)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "0ef906dd-d70a-4e15-a1f2-c1fd1062e575")
	)
	(fp_line
		(start -6.25 2.5)
		(end -6.75 2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "c12b4436-779d-443b-b3bd-5ad01684f54f")
	)
	(fp_line
		(start -6.25 6.25)
		(end -6.75 6.25)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "1a7065dd-de7f-48f6-9033-91e64b13afc2")
	)
	(fp_line
		(start 6.25 -6.25)
		(end 6.75 -6.25)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "a117430c-c8ff-4bda-b671-f7a2865669d4")
	)
	(fp_line
		(start 6.25 -2.5)
		(end 6.75 -2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "a3718502-6efc-453e-ba13-d033180aab27")
	)
	(fp_line
		(start 6.25 6.25)
		(end 6.75 6.25)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "6b040489-9023-4f31-935d-7d86a39d0732")
	)
	(fp_line
		(start 6.75 -6.25)
		(end 6.75 -2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "92c791bb-6360-427f-8602-42c071ef7e81")
	)
	(fp_line
		(start 6.75 -2.5)
		(end 6.75 2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "6a41d024-145f-4e5a-87bd-b7a7d9281a09")
	)
	(fp_line
		(start 6.75 -2.5)
		(end 7 -2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "beb8e98a-34d7-4d6d-b8b3-6cdf38882b04")
	)
	(fp_line
		(start 6.75 2.5)
		(end 6.25 2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "e6a5e2ec-fa5d-46e5-aea8-b17d9266f7c6")
	)
	(fp_line
		(start 6.75 6.25)
		(end 6.75 2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "0d6208f3-4ae8-44c5-af1e-82b54d1174c0")
	)
	(fp_line
		(start 7 -2.5)
		(end 7 2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "54194e9f-3fe0-4cc8-856f-a773b9ed771c")
	)
	(fp_line
		(start 7 2.5)
		(end 6.75 2.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.Fab")
		(uuid "99199f42-7368-4136-8f5e-87835693baa6")
	)
	(fp_rect
		(start -6.25 -6.25)
		(end 6.25 6.25)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.Fab")
		(uuid "b34fda5f-d764-4f33-833f-e5eee2481650")
	)
	(pad "" smd roundrect
		(at -6.25 -1.75)
		(size 1.3 1.5)
		(layers "F.Paste")
		(roundrect_rratio 0.1538461538)
		(zone_connect 2)
		(teardrops
			(best_length_ratio 0.3)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "73e9ddab-135e-43f0-b94e-f294f7dd52cd")
	)
	(pad "" smd roundrect
		(at -6.25 0)
		(size 1.3 1.5)
		(layers "F.Paste")
		(roundrect_rratio 0.1538461538)
		(zone_connect 2)
		(teardrops
			(best_length_ratio 0.3)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "901e6f5a-d0f7-4bfe-a954-a14120a27508")
	)
	(pad "" smd roundrect
		(at -6.25 1.75)
		(size 1.3 1.5)
		(layers "F.Paste")
		(roundrect_rratio 0.1538461538)
		(zone_connect 2)
		(teardrops
			(best_length_ratio 0.3)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "b769fa2f-38e6-474a-a262-a038be702fd6")
	)
	(pad "" smd roundrect
		(at -4.75 -1.75)
		(size 1.3 1.5)
		(layers "F.Paste")
		(roundrect_rratio 0.1538461538)
		(zone_connect 2)
		(teardrops
			(best_length_ratio 0.3)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "7a936165-8e60-4c14-a257-8233c0c524e8")
	)
	(pad "" smd roundrect
		(at -4.75 0)
		(size 1.3 1.5)
		(layers "F.Paste")
		(roundrect_rratio 0.1538461538)
		(zone_connect 2)
		(teardrops
			(best_length_ratio 0.3)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "00ad49bf-6c30-41b0-9fe4-553ab8c55ab7")
	)
	(pad "" smd roundrect
		(at -4.75 1.75)
		(size 1.3 1.5)
		(layers "F.Paste")
		(roundrect_rratio 0.1538461538)
		(zone_connect 2)
		(teardrops
			(best_length_ratio 0.3)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "5d965e99-3c99-4d2c-b00a-78b2cf81bdf2")
	)
	(pad "" smd roundrect
		(at 0 -4.75)
		(size 10.5 2)
		(layers "F.Adhes")
		(roundrect_rratio 0.25)
		(uuid "0854bdd0-d544-4a71-b30a-cef345af5c3f")
	)
	(pad "" smd roundrect
		(at 0 0 90)
		(size 5.5 5.5)
		(layers "F.Adhes")
		(roundrect_rratio 0.09090909091)
		(uuid "ca0d2709-fb2a-4362-9b01-6aff19ad51d3")
	)
	(pad "" smd roundrect
		(at 0 4.75)
		(size 10.5 2)
		(layers "F.Adhes")
		(roundrect_rratio 0.25)
		(uuid "a075eb3c-66e4-41af-861b-9b4b8c4cea06")
	)
	(pad "" smd roundrect
		(at 4.75 -1.75)
		(size 1.3 1.5)
		(layers "F.Paste")
		(roundrect_rratio 0.1538461538)
		(zone_connect 2)
		(teardrops
			(best_length_ratio 0.3)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1b2296fc-8fb7-4cb6-964c-497a4b69a0cb")
	)
	(pad "" smd roundrect
		(at 4.75 0)
		(size 1.3 1.5)
		(layers "F.Paste")
		(roundrect_rratio 0.1538461538)
		(zone_connect 2)
		(teardrops
			(best_length_ratio 0.3)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "7978ba1b-f003-41a3-a030-a54924a3d9cc")
	)
	(pad "" smd roundrect
		(at 4.75 1.75)
		(size 1.3 1.5)
		(layers "F.Paste")
		(roundrect_rratio 0.1538461538)
		(zone_connect 2)
		(teardrops
			(best_length_ratio 0.3)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "99d715fa-8fc7-4388-bfaa-f0fe88b9234d")
	)
	(pad "" smd roundrect
		(at 6.25 -1.75)
		(size 1.3 1.5)
		(layers "F.Paste")
		(roundrect_rratio 0.1538461538)
		(zone_connect 2)
		(teardrops
			(best_length_ratio 0.3)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "3c26f7ea-d47a-41f2-b6d5-0c510a3b1034")
	)
	(pad "" smd roundrect
		(at 6.25 0)
		(size 1.3 1.5)
		(layers "F.Paste")
		(roundrect_rratio 0.1538461538)
		(zone_connect 2)
		(teardrops
			(best_length_ratio 0.3)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "b8321c9e-584a-4540-b004-9eb848c061b2")
	)
	(pad "" smd roundrect
		(at 6.25 1.75)
		(size 1.3 1.5)
		(layers "F.Paste")
		(roundrect_rratio 0.1538461538)
		(zone_connect 2)
		(teardrops
			(best_length_ratio 0.3)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "69e98d4d-2a26-49a8-9ef8-6a1383fc03e7")
	)
	(pad "1" smd roundrect
		(at -5.525 0)
		(size 3.25 5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.05)
		(chamfer_ratio 0.05)
		(chamfer top_right bottom_right)
		(zone_connect 2)
		(teardrops
			(best_length_ratio 0.3)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "540b8482-646b-4fa0-b4be-bf0c094134f7")
	)
	(pad "2" smd roundrect
		(at 5.525 0)
		(size 3.25 5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.05)
		(chamfer_ratio 0.05)
		(chamfer top_left bottom_left)
		(zone_connect 2)
		(teardrops
			(best_length_ratio 0.3)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 2)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "6c20ebd2-046b-468d-bcc7-23c82c065b0f")
	)
	(model ":KICAD7_3DMODEL_DIR:Inductor_SMD.3dshapes/SRP1265C SERIES.stp"
		(offset
			(xyz 0 0 3.75)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -180 0 90)
		)
	)
)
