(footprint "JST_SH_BM07B-SRSS-TB_1x07-1MP_P1.00mm_Vertical"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "JST SH series connector, BM07B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
	(tags "connector JST SH vertical")
	(property "Reference" "J30"
		(at 0 -3.3 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "90d62944-5a60-485e-852b-6508efa97210")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "NAV"
		(at 0 3.3 0)
		(layer "F.Fab")
		(uuid "f4153131-b7b6-41ab-a787-2fdd23b31a00")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "Connector_JST:JST_SH_BM07B-SRSS-TB_1x07-1MP_P1.00mm_Vertical"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5c3e150a-ac34-49f8-9d4e-3c2d0b1f7bdb")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e38bc5ba-c85f-475e-883e-ef3e49bb5d09")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "593e5824-2f4f-4a78-99bb-d65f3dbf83bb")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C160394"
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "173cd834-2c9f-4a5d-9673-d5577412ead6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "JST"
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "262f3b89-475d-408c-8069-1cc1cb5ce5b1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "BM08B-SRSS-TB(LF)(SN)"
		(at 0 0 -90)
		(layer "F.Fab")
		(hide yes)
		(uuid "99d4f194-fd6d-4cc0-9957-595cca8980b9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "JLCPCB_PreferredPart" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5689f3d1-3697-4b03-9f5e-a7043763f964")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "JLCPCB_StandardOnly" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6e3d1175-e6f4-4ba4-b4ad-2fac8c57e066")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -4.61 -0.04)
		(end -4.61 1.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2be798be-efd2-4802-bbed-3d29156f62af")
	)
	(fp_line
		(start -4.61 1.11)
		(end -3.56 1.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "618210f8-d5a2-4906-8d1e-c910c89eed8e")
	)
	(fp_line
		(start -3.56 1.11)
		(end -3.56 2.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3daec07b-4325-43ca-bd89-d37c0f97e720")
	)
	(fp_line
		(start -3.44 -2.01)
		(end 3.44 -2.01)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "173b74a3-509e-4c72-b3a4-d23a74018875")
	)
	(fp_line
		(start 4.61 -0.04)
		(end 4.61 1.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d3d20e8d-7e95-425a-bec5-b64177c186af")
	)
	(fp_line
		(start 4.61 1.11)
		(end 3.56 1.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "bdb541f0-61ba-4094-af37-e71306c68e8a")
	)
	(fp_line
		(start -5.4 -2.6)
		(end -5.4 2.6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "5fffc93f-01e5-4a6f-b90e-c302d339833b")
	)
	(fp_line
		(start -5.4 2.6)
		(end 5.4 2.6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "39e55718-eb7b-45d5-b6ea-458246c02d2d")
	)
	(fp_line
		(start 5.4 -2.6)
		(end -5.4 -2.6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a10dd823-6848-44b1-b849-40628c9c4c71")
	)
	(fp_line
		(start 5.4 2.6)
		(end 5.4 -2.6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a68829af-89f9-488e-b5a1-70785b916d86")
	)
	(fp_line
		(start -4.5 -1.9)
		(end 4.5 -1.9)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "874a48b5-29d5-4245-bd64-dbc7c4095935")
	)
	(fp_line
		(start -4.5 1)
		(end -4.5 -1.9)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c48976f2-69ea-495e-85fa-3d25edda00fb")
	)
	(fp_line
		(start -4.5 1)
		(end 4.5 1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "aa0b5606-c859-4fb1-806a-9407d07cb859")
	)
	(fp_line
		(start -3.5 1)
		(end -3 0.292893)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "93e6fd06-f959-4cca-b963-5dc7df855e0c")
	)
	(fp_line
		(start -3.15 -1.55)
		(end -3.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f1a92696-7406-4aa7-83a9-e1bc15f8646d")
	)
	(fp_line
		(start -3.15 -0.95)
		(end -2.85 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f689389c-c38f-47d0-8b52-6d966b1d4144")
	)
	(fp_line
		(start -3 0.292893)
		(end -2.5 1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3babd8e8-3f16-4ac1-90a4-f7c7f3a4fbc6")
	)
	(fp_line
		(start -2.85 -1.55)
		(end -3.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1c7fcdf0-4b95-4ebb-b05c-7e31274b6fd4")
	)
	(fp_line
		(start -2.85 -0.95)
		(end -2.85 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "74fa3415-176a-4237-89f2-139447b56529")
	)
	(fp_line
		(start -2.15 -1.55)
		(end -2.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0c5682be-1736-4093-bda1-5bb585f478ea")
	)
	(fp_line
		(start -2.15 -0.95)
		(end -1.85 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "efcbf3f2-fe86-47cc-91b6-3729cf0bccb9")
	)
	(fp_line
		(start -1.85 -1.55)
		(end -2.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "74f82f62-db74-4d8a-9a9a-911d4d2b59c8")
	)
	(fp_line
		(start -1.85 -0.95)
		(end -1.85 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "00504493-e3c0-4f29-835c-a7f15e617f02")
	)
	(fp_line
		(start -1.15 -1.55)
		(end -1.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "752c5cf1-3c22-4b98-b445-096c9dd9a2ad")
	)
	(fp_line
		(start -1.15 -0.95)
		(end -0.85 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f60e04f7-7beb-4191-92c3-0bcd0f8cb400")
	)
	(fp_line
		(start -0.85 -1.55)
		(end -1.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "94a175af-1663-4c11-b56d-130d055cd369")
	)
	(fp_line
		(start -0.85 -0.95)
		(end -0.85 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5cf22b27-32d9-4303-816c-4f80b9c08e3b")
	)
	(fp_line
		(start -0.15 -1.55)
		(end -0.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2b28508f-367b-46e4-b4e7-e47ad7681ed4")
	)
	(fp_line
		(start -0.15 -0.95)
		(end 0.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8cf8c201-be83-42f1-bc32-9a882e82439a")
	)
	(fp_line
		(start 0.15 -1.55)
		(end -0.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "28c47630-996a-4a24-ab77-d504190c6368")
	)
	(fp_line
		(start 0.15 -0.95)
		(end 0.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b9ac84e7-4da3-41f0-b5bf-025e58d29714")
	)
	(fp_line
		(start 0.85 -1.55)
		(end 0.85 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "be2ae62e-66e8-48e4-a0d4-8b5b6f495b91")
	)
	(fp_line
		(start 0.85 -0.95)
		(end 1.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a75ac590-568f-4ba3-9fe3-a882d56bdd2b")
	)
	(fp_line
		(start 1.15 -1.55)
		(end 0.85 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a8356fa7-8d8e-4e8e-af03-6213db3f1053")
	)
	(fp_line
		(start 1.15 -0.95)
		(end 1.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "bf1cebeb-dca2-40ad-be54-96c293a7b909")
	)
	(fp_line
		(start 1.85 -1.55)
		(end 1.85 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e5f60b80-016c-40cd-8442-0e0710fe7781")
	)
	(fp_line
		(start 1.85 -0.95)
		(end 2.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6dea6cb9-e874-4564-9bb7-2ff5263f6118")
	)
	(fp_line
		(start 2.15 -1.55)
		(end 1.85 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0a9647c8-c849-4592-892b-e2e0a8e5cb81")
	)
	(fp_line
		(start 2.15 -0.95)
		(end 2.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0b48025c-f658-4659-9f53-06993ab56053")
	)
	(fp_line
		(start 2.85 -1.55)
		(end 2.85 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c95ca618-8f8b-4519-a3b5-40f2d1139c8a")
	)
	(fp_line
		(start 2.85 -0.95)
		(end 3.15 -0.95)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7d457dd1-6bea-4479-af23-f8a367af6537")
	)
	(fp_line
		(start 3.15 -1.55)
		(end 2.85 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a6ef0adb-e12e-428e-a8be-1ba7be4ee54a")
	)
	(fp_line
		(start 3.15 -0.95)
		(end 3.15 -1.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c7ebb6f4-e783-4990-932f-41e4271ddc6a")
	)
	(fp_line
		(start 4.5 1)
		(end 4.5 -1.9)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "83b6bde0-d1d9-46ae-ba5b-58f19fc1b551")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -0.25 0)
		(layer "F.Fab")
		(uuid "d26b735c-94df-4851-8299-7f06bc395208")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -3 1.325)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "8c0b50fb-7658-4d2f-9dd5-f02bc67c84a4")
	)
	(pad "2" smd roundrect
		(at -2 1.325)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "9a64ad48-b9d5-4338-a261-69374da2ed1e")
	)
	(pad "3" smd roundrect
		(at -1 1.325)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "6cd7b56a-f88f-41a6-a240-9f0a143671a5")
	)
	(pad "4" smd roundrect
		(at 0 1.325)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "117af807-0ca1-4f54-bfb9-59637758be40")
	)
	(pad "5" smd roundrect
		(at 1 1.325)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "c49200d8-ae8e-4a06-bc99-c9fa91db3f45")
	)
	(pad "6" smd roundrect
		(at 2 1.325)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "532cc1dd-671e-42d7-9e24-997bac3003e2")
	)
	(pad "7" smd roundrect
		(at 3 1.325)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(uuid "71fbbb43-57e1-4565-893e-8a370c05e139")
	)
	(pad "MP" smd roundrect
		(at -4.3 -1.2)
		(size 1.2 1.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.208333)
		(uuid "aa494fb4-aebc-4486-a942-a33896a54f2f")
	)
	(pad "MP" smd roundrect
		(at 4.3 -1.2)
		(size 1.2 1.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.208333)
		(uuid "50f203a8-6b0e-488b-bddb-13592c40b42c")
	)
	(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_BM07B-SRSS-TB_1x07-1MP_P1.00mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_BM07B-SRSS-TB.STEP"
		(offset
			(xyz 0 0.45 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
