(footprint "TI_Q5DC"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Texas Instruments Q5DC package for CSD88599Q5DC")
	(tags "CSD88599Q5DC Q5DC TI Texas")
	(property "Reference" "Q1"
		(at 0 -3.9 180)
		(layer "F.SilkS")
		(hide yes)
		(uuid "f26bfd45-e374-49ef-8f8d-6d3dc3409c4f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "TI_CSD88599Q5DC"
		(at 0 3.4 180)
		(layer "F.Fab")
		(uuid "e4233522-703c-4e1d-912c-5bfda30fcb71")
		(effects
			(font
				(size 0.25 0.25)
				(thickness 0.05)
			)
		)
	)
	(property "Footprint" "Package_DFN_QFN:TI_Q5DC"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "474bcf41-a6d0-4401-800d-cf9b278804ef")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "aad50af8-295b-43c0-8b97-9f890143cf12")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1e01ed8d-036d-448d-8716-86ab4a2ac1b9")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "LCSC" "C2871380"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "3e32f210-1ce2-4e74-9a83-6f3826bb6428")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MFG" "TI"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "d679cc08-1e4c-4136-aa1a-e01766da7196")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "MPN" "CSD88599Q5DC"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "446f6d4e-ebae-4db9-a512-dd079e64a194")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Preferred" ""
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "08669fea-185d-4ebb-a444-de39661f4c7a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Field-1" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d80b2bdc-2409-46f4-828d-ba1557a32044")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(solder_mask_margin 0.07)
	(attr smd)
	(fp_line
		(start -2.75 -3.25)
		(end -2.75 -2.8)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ed193568-3329-452f-a77d-1e0be6eada36")
	)
	(fp_line
		(start -2.75 -3.25)
		(end -2.5 -3.25)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4f18ca55-722d-4783-b1bc-2a20241e6449")
	)
	(fp_line
		(start -2.75 3.25)
		(end -2.75 2.8)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "84ffe05b-055e-4c82-96e1-02839a1dd390")
	)
	(fp_line
		(start -2.75 3.25)
		(end -2.5 3.25)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "61d1b836-0eab-4b8b-8554-2debdea933ad")
	)
	(fp_line
		(start 2.75 -3.25)
		(end 2.5 -3.25)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f3cef083-0240-4ede-af26-7a318ef6c6ae")
	)
	(fp_line
		(start 2.75 -3.25)
		(end 2.75 -2.8)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c4d1581c-509a-4de3-bcaf-9f69c7eaf508")
	)
	(fp_line
		(start 2.75 3.25)
		(end 2.5 3.25)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ce6a8fb2-5ed7-4cff-a790-294f4be7c7d4")
	)
	(fp_line
		(start 2.75 3.25)
		(end 2.75 2.8)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a7f122ae-fe1b-4677-ab6e-a1d582955be8")
	)
	(fp_circle
		(center -3 -3.2)
		(end -3 -3.25)
		(stroke
			(width 0.15)
			(type solid)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "248b28bf-713d-41ec-93cd-2681457242aa")
	)
	(fp_line
		(start -2.85 2.575)
		(end -2.85 -2.575)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9dcc1432-1512-463d-92d2-c6a2d3ea6aef")
	)
	(fp_line
		(start -2.75 -3)
		(end -2.749228 -2.748649)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "703a2090-542e-4006-959e-4e32296d4a78")
	)
	(fp_line
		(start -2.75 3)
		(end -2.749228 2.748649)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "d977834e-5b59-44af-b4e0-4d44db413668")
	)
	(fp_line
		(start -2.5 -3.25)
		(end -2.43309 -3.255779)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "11c7ef5c-aafc-4b08-97e5-c9463b1bbd77")
	)
	(fp_line
		(start -2.5 3.25)
		(end -2.43309 3.255779)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "226ed253-d9a5-4dc9-bd82-ecac1d245754")
	)
	(fp_line
		(start -2.25 -3.35)
		(end 2.25 -3.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "38b7b9e4-74fb-417c-947d-7218000e9db3")
	)
	(fp_line
		(start 2.25 3.35)
		(end -2.25 3.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f7476561-ca07-42cd-b382-4b07822ca128")
	)
	(fp_line
		(start 2.5 -3.25)
		(end 2.43309 -3.255779)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "f018b5ff-ca15-4129-8c01-b9ca7833e2c0")
	)
	(fp_line
		(start 2.5 3.25)
		(end 2.43309 3.255779)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "59cc5069-463c-423e-adcf-3a65f3540895")
	)
	(fp_line
		(start 2.75 -3)
		(end 2.749228 -2.748649)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "c8db8e6e-2c57-4a6b-8a53-664bd52e0618")
	)
	(fp_line
		(start 2.75 3)
		(end 2.749228 2.748649)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "c71edc2d-efdf-4f9b-91d3-ceb5ab32cf97")
	)
	(fp_line
		(start 2.85 -2.575)
		(end 2.85 2.575)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "4d9735f3-f2d3-45a9-b07e-8e63d7da0f97")
	)
	(fp_arc
		(start -2.85 -2.575)
		(mid -2.822982 -2.675385)
		(end -2.749228 -2.748649)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ca44c244-79ac-44d4-9650-2555134722f9")
	)
	(fp_arc
		(start -2.75 -3)
		(mid -2.676777 -3.176777)
		(end -2.5 -3.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "d998684c-b291-4271-b176-e396309498c2")
	)
	(fp_arc
		(start -2.749228 2.748649)
		(mid -2.822982 2.675385)
		(end -2.85 2.575)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "cc20c221-16fb-44d3-bcdc-853327d60dd6")
	)
	(fp_arc
		(start -2.5 3.25)
		(mid -2.676777 3.176777)
		(end -2.75 3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "bf5ef1d0-fa6a-42d1-8548-acd483388245")
	)
	(fp_arc
		(start -2.43309 -3.255779)
		(mid -2.352956 -3.325063)
		(end -2.25 -3.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "18a610bf-2fe4-4d48-a17b-a44be959a042")
	)
	(fp_arc
		(start -2.25 3.35)
		(mid -2.352956 3.325063)
		(end -2.43309 3.255779)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5264d130-5618-4741-8323-2aee9583dc27")
	)
	(fp_arc
		(start 2.25 -3.35)
		(mid 2.352956 -3.325063)
		(end 2.43309 -3.255779)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "bf1a4a3e-a3db-4337-9947-8b1184bc61cd")
	)
	(fp_arc
		(start 2.43309 3.255779)
		(mid 2.352956 3.325063)
		(end 2.25 3.35)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "886844e8-cfff-4551-ad0f-b0f05d61ccd2")
	)
	(fp_arc
		(start 2.5 -3.25)
		(mid 2.676777 -3.176777)
		(end 2.75 -3)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9573cb0a-a610-4c8d-b569-42a397d01e69")
	)
	(fp_arc
		(start 2.749228 -2.748649)
		(mid 2.822982 -2.675386)
		(end 2.85 -2.575)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "19846be8-8112-45a7-abf8-73efff3a1ade")
	)
	(fp_arc
		(start 2.75 3)
		(mid 2.676777 3.176777)
		(end 2.5 3.25)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "c6305eaf-8c64-4627-b554-d997ede1cf1a")
	)
	(fp_arc
		(start 2.85 2.575)
		(mid 2.822982 2.675385)
		(end 2.749228 2.748649)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "d2a86128-85a9-4751-afc4-05dacbf1f9c9")
	)
	(fp_line
		(start -2.5 -3)
		(end 2.5 -3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "27471fc0-1da2-4ba6-81c2-45c21a2af1bf")
	)
	(fp_line
		(start -2.5 3)
		(end -2.5 -3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f4a30b2f-9a6f-4dd9-9785-7ff9f3b539cb")
	)
	(fp_line
		(start 2.5 -3)
		(end 2.5 3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8b1731d9-106e-407e-8536-e4a4d8e98563")
	)
	(fp_line
		(start 2.5 3)
		(end -2.5 3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "56c9c2e1-7d34-4fdd-8e7d-13c27a4f0933")
	)
	(pad "" smd roundrect
		(at -0.81 -1.98)
		(size 1.41 1.12)
		(layers "F.Paste")
		(roundrect_rratio 0.089)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "c2ea980f-1f01-4bf9-9de1-9143d1b8fde5")
	)
	(pad "" smd roundrect
		(at -0.81 -0.66)
		(size 1.41 1.12)
		(layers "F.Paste")
		(roundrect_rratio 0.089)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "13ecc42c-b3e5-4e5b-9a76-502e1b6a0cd1")
	)
	(pad "" smd roundrect
		(at -0.81 0.66)
		(size 1.41 1.12)
		(layers "F.Paste")
		(roundrect_rratio 0.089)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "c3ec7bb3-4dd5-4efe-ab6c-147013e64893")
	)
	(pad "" smd roundrect
		(at -0.81 1.98)
		(size 1.41 1.12)
		(layers "F.Paste")
		(roundrect_rratio 0.089)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "5ec37c5c-02e4-4bef-b0c9-42f52893a9a8")
	)
	(pad "" smd roundrect
		(at 0.81 -1.98)
		(size 1.41 1.12)
		(layers "F.Paste")
		(roundrect_rratio 0.089)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "fcd2f1d5-efb3-4310-8b32-5ee72ab5131a")
	)
	(pad "" smd roundrect
		(at 0.81 -0.66)
		(size 1.41 1.12)
		(layers "F.Paste")
		(roundrect_rratio 0.089)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "982621a3-51e3-4b97-a873-ad33b63cf4cd")
	)
	(pad "" smd roundrect
		(at 0.81 0.66)
		(size 1.41 1.12)
		(layers "F.Paste")
		(roundrect_rratio 0.089)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1a94abc9-5191-4424-a25a-aa8e1913a6d5")
	)
	(pad "" smd roundrect
		(at 0.81 1.98)
		(size 1.41 1.12)
		(layers "F.Paste")
		(roundrect_rratio 0.089)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "6801b96f-59d3-4c57-aa0a-67c19275bc4e")
	)
	(pad "GH" smd roundrect
		(at -2.35 -2.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "da3dfe47-9a00-451e-b022-69a064c26cb3")
	)
	(pad "GL" smd roundrect
		(at 2.35 -2.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "9bef2c2a-7a47-4b68-9688-e3c7f63cd1a8")
	)
	(pad "NC" smd roundrect
		(at -2.115 -3.013)
		(size 0.43 0.375)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "517d2e4f-6482-48b4-93a4-f81a083671fa")
	)
	(pad "NC" smd roundrect
		(at -2.115 3.013)
		(size 0.43 0.375)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "41c73be7-c233-4443-bd72-9bc9a139249f")
	)
	(pad "NC" smd roundrect
		(at 2.115 -3.013)
		(size 0.43 0.375)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "1d4d3c1d-1385-467c-92dc-5d321ea509cb")
	)
	(pad "NC" smd roundrect
		(at 2.115 3.013)
		(size 0.43 0.375)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "a1b39819-38df-450d-bde5-d956f4487239")
	)
	(pad "NC" smd roundrect
		(at 2.35 -2)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "5bab8497-4da6-4de7-9e1d-61644a81e3aa")
	)
	(pad "PGND" smd roundrect
		(at 2.15 0.5)
		(size 0.3 4.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "84606589-4570-4ade-9f11-f5f22bee8419")
	)
	(pad "PGND" smd roundrect
		(at 2.35 -1.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "9503f3dc-79dc-4588-a1c6-9c6e7ec805a4")
	)
	(pad "PGND" smd roundrect
		(at 2.35 -1)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "9451b175-a806-4cc4-8e23-c9d6105995fc")
	)
	(pad "PGND" smd roundrect
		(at 2.35 -0.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "55e30824-48c0-4f19-b681-26cd787cf20d")
	)
	(pad "PGND" smd roundrect
		(at 2.35 0)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "0e892c6a-7da6-4d76-b192-ca4432c10c90")
	)
	(pad "PGND" smd roundrect
		(at 2.35 0.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "846960f4-a01e-4e83-815c-d7c21df54be5")
	)
	(pad "PGND" smd roundrect
		(at 2.35 1)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "b2e81141-ac3b-4014-80b7-227e93547da5")
	)
	(pad "PGND" smd roundrect
		(at 2.35 1.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "c1d64f02-8984-4583-bd78-067db8f2b839")
	)
	(pad "PGND" smd roundrect
		(at 2.35 2)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "14f673bd-fc07-4446-a735-b906c707306d")
	)
	(pad "PGND" smd roundrect
		(at 2.35 2.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "e3caa5f6-e8e9-4715-b921-b9909d3629f5")
	)
	(pad "SH" smd roundrect
		(at -2.35 -2)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "bf07efe3-9bf2-44f4-9eae-39c59da1ac40")
	)
	(pad "VIN" smd roundrect
		(at 0 0)
		(size 3.3 5.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.03)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "c3f1f04e-7b8c-4c9b-ba6b-5a123c55c43f")
	)
	(pad "VSW" smd roundrect
		(at -2.35 -1.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "71f89695-d45f-4842-8d98-c1db30e549af")
	)
	(pad "VSW" smd roundrect
		(at -2.35 -1)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "87946d93-3d1a-4344-a0a1-15c359745037")
	)
	(pad "VSW" smd roundrect
		(at -2.35 -0.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "0f39ed34-0446-4cb4-90e5-2f0fb6992017")
	)
	(pad "VSW" smd roundrect
		(at -2.35 0)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "63eb573c-f572-437d-8b95-523628bda23e")
	)
	(pad "VSW" smd roundrect
		(at -2.35 0.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "7feebb57-ae62-4b73-9190-95bdad5998ed")
	)
	(pad "VSW" smd roundrect
		(at -2.35 1)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "9f613822-47bb-49a8-859a-c9ca33c25d23")
	)
	(pad "VSW" smd roundrect
		(at -2.35 1.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "01df76b3-bff2-4250-951b-840c3fee9068")
	)
	(pad "VSW" smd roundrect
		(at -2.35 2)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "4a893166-ee19-4842-acd8-0afa47f5f127")
	)
	(pad "VSW" smd roundrect
		(at -2.35 2.5)
		(size 0.7 0.25)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "119285cf-e0bb-4fa3-affa-70316cee9afa")
	)
	(pad "VSW" smd roundrect
		(at -2.15 0.5)
		(size 0.3 4.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.2)
		(teardrops
			(best_length_ratio 0.33)
			(max_length 0.3)
			(best_width_ratio 1)
			(max_width 0.5)
			(curve_points 10)
			(filter_ratio 0.9)
			(enabled yes)
			(allow_two_segments yes)
			(prefer_zone_connections yes)
		)
		(uuid "dfb590d2-5ba1-40c7-b7f5-05b95fdc0651")
	)
	(model "${KICAD7_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/TI_Q5DC.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)