(module Castellated_Connector_6P (layer F.Cu) (tedit 56FFAEC7)
  (fp_text reference REF** (at -1.5 -1) (layer F.SilkS)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_text value Castellated_Connector_6P (at 0 1) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.125)))
  )
  (fp_line (start -3 0) (end 3 0) (layer Dwgs.User) (width 0.05))
  (pad 1 thru_hole rect (at -2.5 0) (size 0.8 0.8) (drill 0.45) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -1.5 0) (size 0.8 0.8) (drill 0.45) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -0.5 0) (size 0.8 0.8) (drill 0.45) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 0.5 0) (size 0.8 0.8) (drill 0.45) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 1.5 0) (size 0.8 0.8) (drill 0.45) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 2.5 0) (size 0.8 0.8) (drill 0.45) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 0 -1.5) (size 2 2) (drill 2) (layers *.Cu *.Mask))
)
