(module Flat_cable_pads_40P_1.27 (layer F.Cu) (tedit 5C1E0A6E)
  (attr virtual)
  (fp_text reference REF** (at 0 -26.035) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Flat_cable_pads_40P_1.27 (at 3.81 0 270) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.05)))
  )
  (pad 1 connect rect (at 0 -24.765) (size 6.35 1.02) (layers F.Cu F.Mask))
  (pad 2 connect roundrect (at 0 -23.495) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 3 connect roundrect (at 0 -22.225) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 4 connect roundrect (at 0 -20.955) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 5 connect roundrect (at 0 -19.685) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 6 connect roundrect (at 0 -18.415) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 7 connect roundrect (at 0 -17.145) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 8 connect roundrect (at 0 -15.875) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 9 connect roundrect (at 0 -14.605) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 10 connect roundrect (at 0 -13.335) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 11 connect roundrect (at 0 -12.065) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 12 connect roundrect (at 0 -10.795) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 13 connect roundrect (at 0 -9.525) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 14 connect roundrect (at 0 -8.255) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 15 connect roundrect (at 0 -6.985) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 16 connect roundrect (at 0 -5.715) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 17 connect roundrect (at 0 -4.445) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 18 connect roundrect (at 0 -3.175) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 19 connect roundrect (at 0 -1.905) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 20 connect roundrect (at 0 -0.635) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 21 connect roundrect (at 0 0.635) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 22 connect roundrect (at 0 1.905) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 23 connect roundrect (at 0 3.175) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 24 connect roundrect (at 0 4.445) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 25 connect roundrect (at 0 5.715) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 26 connect roundrect (at 0 6.985) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 27 connect roundrect (at 0 8.255) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 28 connect roundrect (at 0 9.525) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 29 connect roundrect (at 0 10.795) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 30 connect roundrect (at 0 12.065) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 31 connect roundrect (at 0 13.335) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 32 connect roundrect (at 0 14.605) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 33 connect roundrect (at 0 15.875) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 34 connect roundrect (at 0 17.145) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 35 connect roundrect (at 0 18.415) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 36 connect roundrect (at 0 19.685) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 37 connect roundrect (at 0 20.955) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 38 connect roundrect (at 0 22.225) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 39 connect roundrect (at 0 23.495) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad 40 connect roundrect (at 0 24.765) (size 6.35 1.02) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
)
